# 5235 Idle Softkeys

## Purpose

The 5235 Idle Softkeys form allows the user to customize the six softkeys of the Mitel 5235 IP Phone. Users can retain the six default softkeys or they can choose Personal Softkeys to replace the defaults. All six keys must be used for either application.

The defaults for the idle softkeys are as follows:

- Phone: Used to access programmable keys and the main phone and call control interface.

- People: Accesses a personal contacts list.

- Messages: Displays the visual voice mail interface used to interact with voice mail system.

- History: Shows a log of missed, made, and answered calls.

- Settings: Used to customize the 5235 IP Phone.

- Applications: Provides a launch point to the Conference Control and Web Browser applications.

Use this form when performing the following tasks:

- Program Personal Softkeys for 5235 IP Phones

## Conditions

- Only the Phone and Application softkeys can be programmed from the System Administration Tool; the others must be programmed from the phone.

- The 5235 IP Phone is no longer supported as of MiVoice Business Release 8.0.

## Field Descriptions

Parameter | Description | Default Value
Prime Directory Number | System-generated, protected field. Indicates the unique directory number of the multiline set, as defined in the Multiline IP Sets form. |
Prime Name | System-generated, protected field. Displays the name associated with the primary directory number. |
Lock Default Configuration | System-generated, protected field. This field indicates that the default idle softkeys are not locked and can be set to Personal Softkeys. | No
Personal Softkeys Selected | Select "Yes" to allow the six Personal Softkeys to be used, rather than the default idle softkeys. The Lock Default Configuration must be set to "No". | No
Idle Softkeys |
Key Number | System-generated, protected field. Contains entries numbered from 1 to 6 to designate the six idle softkeys. |
Key Directory Number | If CDE Speedcall is selected as the Feature Type, use this field to program or delete the CDE Speedcall. To program a CDE speedcall, enter the destination directory number (maximum of 7 digits) in this field. If User Speedcall is selected as the Feature Type, use this field to program or delete non-private user speedcalls. To program a user speedcall, enter the destination directory number (maximum of 26 digits) in this field. If the speedcall is private, the Key Directory Number field displays "xxxxxxx". | Blank
Feature Type | Select a feature name from the feature drop-down list. The feature type defaults to unassigned and deleting a feature causes it to revert to unassigned. COS-dependent features can be configured, but the feature remains inactive if the COS is not enabled. | Not assigned
Label | Enter the name of the feature for the phone label. | Blank