# Call Forward - Delay

## Description

While engaged in a call, the called party has the opportunity to answer an incoming call before the calling party is forwarded to an alternate answer point. The called party hears camp-on tone when there is an incoming call. Display sets also show " XXXX is waiting" (where XXXX is the extension of the calling party). Incoming calls camp-on until the programmed timer runs out. They are then forwarded to the programmed Call Forward No Answer point.

## Conditions and Feature Interactions

- If Call Forward Busy is enabled on the set, incoming calls follow the Call Forward Busy programming and do not camp-on.

- Call Rerouting is not supported for this feature. The call is forwarded after the Call Forward - Delay timer expires only if the Call Forward No Answer feature is configured and enabled for the user, otherwise the call is camped on indefinitely.

## Programming

In the Class of Service Options form :

- Set the Call Forward - Delay (0 - 125 sec) option to the desired time

- Set the Call Forward No Answer Timer (0 - 125 sec) option to the desired time

If this timer is set to "0", the functionality is disabled and calls follow normal programming conditions.

## Device Support

All devices

## Operation

None

Related Topics

- Call Forward