# Programming Analogue FXS Ports

The User and Services Configuration form combines the functions of several system forms into a single form; however, you can still access and use the individual forms.

## Programming

Fill out the form User and Service Configuration to program Analogue FXS Port:

- Click User and Devices > User and Services Configuration from the left navigation pane.

- To add a phone, click Add > select Default User and Device

- Click on the tab User Profile > enter the name

- Click on the tab Service Profile > enter the number. Set the device type to Analog FXS

- Click on the tab Device Details. By default the first Endpoint ID is selected but, you can manually select the required Endpoint ID from the drop down.

- Click Save Changes.