# Programming Analog Music On Hold

## Overview

Analog Music on Hold is provided by an external music source (a radio, for example) connected to any one of the following (see the Hardware Technical Reference Manual for specifications):

- Music on Hold connector on the back of a controller with Embedded Analog

- Music on Hold connector on the back of a Universal ASU

## Programming

To program Music on Hold:

1. System Options form

- Set the Music On Hold option to "Yes".

2. (Optional) Class of Service Options form

- Set Music on Hold on Transfer to "Yes"as desired for each Class of Service.

3. Trunk Circuit Descriptor - E and M form

4. Set the Outgoing Start Type parameter to "Immediate"

5. Set the Transmission Facility parameter to "2 wire"

6. Set the 2 Wire Balanced Network Setting parameter to "600"

7. Set the Perform Seize Test on Out-of-Service Trunks parameter to "No"

8. All other parameters may be any value.

4. E and M Trunks form

- Ensure that the trunk number is unique. The service number, E&M trunk circuit descriptor number, and the interconnect number may be the same as other E&M trunks.

5. System Access Points form

- Set "Music Source" to "External".

- In the "Music Source Port - Location ID" field, enter the PLID of the E&M trunk circuit

  NOTE: Music on Hold can be assigned to either of the first two ports on a Universal ASU E&M card or to the E&M port on the Analog Main Board (AMB) (on a controller with embedded analog). Only one Music on Hold source is permitted per system.

6. If you assigned Music on Hold to an E&M port on the AMB (on a controller with embedded analog) reboot the controller to start Music on Hold operation. Or, if you assigned Music on Hold to a port on a Universal ASU E&M card, reload the Analog Services Unit to start Music on Hold operation.

NOTE: Any omission of programming PLID assignment and or CIM to configured ASU will not permit Music on Hold.

Related Topics

- Music on Hold

- Music on Hold On Transfer