# Configuring User Information
(Mitel Integrated Configuration Wizard)

This page allows you to set the prime contact number, email address, Class of Restriction and UCC Bundle for users. You also assign them a secondary MiVoice Business system for service resiliency
Resilient networks are made up of network elements that provide reliable fail-over mechanisms-either within the device or through working in conjunction with other network elements in order to ensure that all network devices can be used simultaneously. In this way the failure of one device will not bring down the entire network, thereby eliminating single points of failure on the network. A truly resilient network will provide the maximum amount of network uptime without requiring an entire duplicate network. (if applicable).

TIP: You can copy data from an Excel spreadsheet into this page.

1. Select one or more users in the table. Then, click Autofill...

2. Check the Email Address box and enter an email address format to apply to the selected users. You must enter a valid Email address for each MiCollab Audio, Web, and Video user before you can proceed to the next screen.

NOTE: You cannot use accented characters in the First Name, Last Name, Login ID, or email address (for example: š, œ, Ÿ, µ, À, Á, Â, Ã, Ä, Å, Æ, Ç, È, É, Ê, Ë, Ï, Ð, Ñ, Ò, Ó, Ô, Õ, Ö, Ù, Ú, Û, Ü, Ý, à, á, â, ã, ä, å, æ, ç, è, é, ê, ë, ì, í, î, ï, ð, ñ, ò, ó, ô, õ, ö, ù, ú, û, ü, ý.).

3. Check the Class of Restriction box and select a COR to apply to the selected users.

4. (Optional) Select a Secondary MiVoice Business for each user that requires service resiliency
   Resilient networks are made up of network elements that provide reliable fail-over mechanisms-either within the device or through working in conjunction with other network elements in order to ensure that all network devices can be used simultaneously. In this way the failure of one device will not bring down the entire network, thereby eliminating single points of failure on the network. A truly resilient network will provide the maximum amount of network uptime without requiring an entire duplicate network..
   This option is only available when provisioning a cluster
   Refers to a grouping of systems (for example, a cluster MiVoice Business systems) that share common dialing plans, or common directory information, such as Remote Directory Numbers with Telephone Directory..

5. Check the UCC Bundle box and select a UCC licensing bundle to apply to the selected users.

NOTE: The recommended "best practice" is to configure users using Roles and Templates in the MiCollab Users and Services application. Although MiCW allows you to assign UCC bundles, you must assign the correct service mix that is provided in the bundle to each user. In addition, MiCW assigns all NuPoint voicemail users with Standard Unified Messaging. If the assigned UCC Bundle includes entitlement to Advanced Unified Messaging, you must enable it through the MiCollab User and Services application.

6. Click Apply.

7. Click Next to continue.