# Configuring RAD Greetings
(Embedded Voice Mail)

## Overview

You can assign different greeting sets to each one of the 30 RAD greeting sets.

## Programming

To configure RAD greeting sets:

1. Record the greeting using the administrators mailbox or upload the recording file using the System Audio Files Update form.

2. VM Greetings form

3. Assign the RAD set to a voice mail port (for example, RAD Set 10 to Port ID 1).

3. VM RAD Greetings form

- Assign the number of the greeting recordings (1 to 200) to the RAD greeting set.

- Enter how many times the greeting set will be played.

Related Topics

- About Voice Mail

- RAD Greetings

- Program RAD Greetings

- Recording Greetings

- System Audio Files Update

- Tips for Recording Greetings