# L2 STATUS MACLIST

## Qualifiers:

<port_number>

## Purpose:

Lists the MAC addresses of devices connected to the Layer 2 ports and the VLAN it belongs to.

NOTE: This maintenance command is not applicable to MiVoice Business for Industry Standard Servers (ISS).

## Details:

Entering the command without a qualifier displays addresses for all ports. Specifying a port number shows the address for that port.

## Example:

### Entry: L2 STATUS MACLIST

System Response:

Layer 2 Switch MAC Address Forward Table:

Note the list shows the MAC address followed by the VLAN it belongs to.

Port G0

00:01:e7:0b:89:81(0001) 00:04:80:23:39:00(0001) 08:00:0f:00:9b:06(0001)

08:00:0f:00:a2:8a(0001)

Port MMC-C0-0

08:00:0f:19:ab:0a(0001)

Port MMC-C1-0

08:00:0f:19:ab:16(0001)

Port MIPS

08:00:0f:1b:3e:f8(0001)