# Call Forward - Override

## Description

Call Forward Override lets you bypass any Call Forward condition that is set at the station that you are calling.

## Conditions and Feature Interactions

- See Call Forward.

- You must activate Call Forward Override each time that you attempt to bypass Call Forward.

## Programming

1. Complete programming in Call Forward.

2. Class of Service Options form

- Enable Call Forwarding - Override.

3. Feature Access Codes form

- Enter a code for Call Forwarding - Override.

## Device Support

- Supported on all devices.

## Operation

#### 2500, Mitel telephones, and 5560 IPT

To use Call Forward Override:

1. Lift the handset or select the prime line.

2. Dial the Call Forward - Override feature access code.

3. Dial the number.

NOTE: You can also press a DSS key instead of dialing the destination number or a speedcall key containing the destination number. When the DSS key is used in this way, the state of the monitored line is ignored and there is no attempt to perform a DSS pickup of a ringing line.

#### Symbol NetVision Phone

To use Call Forward Override:

1. Press SND.

2. Dial the Call Forward - Override feature access code.

3. Dial the number.

#### Symbol MiNET Wireless Phone

To use Call Forward Override:

1. Press the Send Key.

2. Dial the Call Forward - Override feature access code.

3. Dial the number.

#### OpenPhone 27

To use Call Forward Override:

1. Press .

2. Dial the Call Forward - Override feature access code.

3. Dial the number.

#### SpectraLink Wireless Telephones

To use Call Forward Override:

1. Press .

2. Dial the Call Forward - Override feature access code.

3. Dial the number.

Related Topics

- Call Forward