# Hardware Modules

## Purpose

### 3300 ICP Controller

For a 3300 ICP Controller, the Hardware Modules form displays details about the various cards installed in the 3300 ICP controller. Use this form to perform the following tasks:

- Program Controller Modules

- Controller Module Configuration

### EX Controller

For an EX Controller, the Hardware Modules displays details about the modules installed in the EX controller.

## Conditions

### 3300 ICP Controller

None

### EX Controller

1. If Slot 1 is empty, then no other card is detected and all the slots are shown as empty.

2. If there is an empty slot before a PRI or DSP card, the empty slot will display the following error message - ERROR: An empty slot before a PRI or DSP card is not allowed.

## Field Descriptions

Parameter | Description
Slot Number | System-generated, protected field. The location of the module.
Module ID, Driver ID | System-generated, protected field. Shows the Module ID and the Driver ID, if available.
Minimum Reset Timing | System-generated, protected field. Shows the time required to reset the card, if available.
Card Description | System-generated, protected field. Provides engineering information on the type of card that is installed. 3300 ICP Controller: T1/E1-DSP-VEC-Stratum4Module = T1/E1 Combo card Dual FIM - Multimode 820nm = Dual FIM (not CX II/CXi II)) MT9074 Framer Chip = Dual Framer module (not CX II/CXi II) BRI - S/T Interface - 4 circuit = Quad BRI Framer (not in NA) 8 CCT DSP II / PCB ASSEBLY 56007581 (DSP II MMC, Part No. 50005751) 2 SHARC 21363 DSP (embedded on MXe III and CX II mainboard) 4 SHARC 21161 DSP (Quad DSP MMC; Part No. 50002979; embedded on CX II/CXi II mainboard) 4 SHARC 21262 DSP (all AX controllers) Echo Cancellation 128 Channels = Echo canceller (not CX II/CXi II) EX Controller: PRI (for E1 or T1) FXS FXO DSP (required when system has FXS or FXO)
PCB Assembly | System-generated, protected field. Shows the assembly number of the card, if available.
PCB Revision Level | System-generated, protected field. Shows the revision level of the card, if available.
Processor Type | System-generated, protected field. Provides information on the processor if one is on the card. When there is no processor, this field will display n/a.
Processor Speed (Core, Clock) | System-generated, protected field. Provides information on the speed of the processor if one is on the card. When there is no processor this field will display n/a.
MAC Address | System-generated, protected field. This field will display MAC address, if available.
Country Code | System-generated, protected field. Displays the country for which the card was designed, if available.
Variant ID | System-generated, protected field. This field identifies the card assembly revision, if available.
Serial Number | System-generated, protected field. This field identifies the serial number of the card, if available.