# Bandwidth Management - Configuration Data is Shared via SDS

Because the configuration data for Bandwidth Management applies to all ICPs in the network that require Call Admission Control, you can enter the configuration data into one network element and the System Data Synchronization (SDS) feature shares the data with all the other elements.

See the Bandwidth Management section in SDS Application Specific Guidelines and Limitations for details about the forms that are shared.

Related Topics

- Introduction

- About Zones and ZAPs

- About Call Admission Control

- What Features are Supported?