# Lines Alarm

## System/Sub-System

MiVoice Business: Hardware

## Description

Indicates the amount of stations unavailable as a percentage (%) of the system total. The following are included in the line total:

- All IP devices with a programmed DN in the Multiline Sets, Single Line Sets, Console forms, and Hot Desk Users.

- All ONS devices in the Analog Sets form (whether programmed with a DN or not) associated with an ASU.

- All paging devices programmed in the Loudspeaker Paging form.

- All PKMs.

- All IP music sources (as of 3300 ICP Release 7.0, all systems by default are assigned 64 virtual Music on Hold circuits for embedded MOH, which are included in the count).

Maintenance commands are valid for this alarm.

## Alarm Status

The minor threshold is > 0. The major threshold is 20. The critical threshold is 100.

#### Possible Cause | #### Corrective Action
--- | ---
Check the status of the analog devices. These could reside on the AS. Check the status of your embedded voicemail ports Check the status of your Music on Hold Sources. | Investigate