# Test Error Messages

If errors occur, the details of the error are described in the "Other" column of the test report.

## LS Measure Tool Error Messages

Error (displayed in Other field) | Meaning and Corrective Action
--- | Test was successful. No problems were detected with the trunk.
LOADED LOOP | Test was successful. It is possible that this is a loaded loop. Re-configure the LS Measure tool to test all 5 coefficient settings (instead of just the first 4). Run the test again. If the fifth coefficient is a better match, it will be presented as the recommended setting.
NOT CONFIGD | The circuit is not configured, or it is not IDLE. Please check that the trunk is programmed correctly and an ASU is connected to the CIM port.
CAN'T SEIZE | LS Measure tool could not seize the specified trunk. Ensure that the trunk is in the IDLE state.
NO DIAL TONE | Dial tone was not detected. The LS Measure Tool seized the trunk but was unable to detect dial tone to make the outgoing call to the CO. Make sure an ASU is connected to the CIM port and that the ASU is programmed. Also make sure the specified LS port is connected to CO.
ERR DIALING | There was a problem outpulsing the DTMF digits to the CO. Ensure that the milliwatt tone and silence numbers are valid. Entering # or * in the digit sequence will cause this error.
ERR RECORD | The LS Measure Tool was waiting for a signal from the CO, but never received it. Ensure that the milliwatt tone and silence numbers are valid.
ERR RELEASE | The test failed. The LS Measure Tool tried to release the trunk, but failed. Make sure the ASU is connected to the CIM port and that the ASU is still programmed. Also make sure the specified LS port is still physically connected to CO.
STATE ERROR | The test failed due to a port state machine problem (wrong state)! There was an internal error with the LS Measure Tool. Restart the LS Measure Tool.

Related Topics

- Measuring LS Trunk Line Settings

- Individual or Batch line quality test

- Individual or Batch Distortion Echo Test

- Program Analog Trunks