# SMDR - Summary of Fields Tables

The following options affect the length of an SMDR record and the fields recorded:

- Extended Digit Length (see the Extended Digit Length Record Fields table)

- ANI/DNIS/ISDN/CLASS Number Delivery Reporting (see the Standard SMDR Record Fields table and the Extended Digit Length Record Fields table)

- Standardized Network OLI (see the Standard SMDR Record Fields table and the Extended Digit Length Record Fields table)

- Extended Reporting Level 1

- Extended Reporting Level 1 and Level 2

The following SMDR options affect the format of certain SMDR record fields:

- Extended Time to Answer (see the Extended Time To Answer SMDR Record Fields table)

- Network Format (see the Standard SMDR Record Fields table and the Extended Digit Length Record Fields table)

## Standard SMDR Record Fields

The table below provides an overview of the basic SMDR fields when Extended Digit Length and Extended Time to Answer are NOT enabled.

The standard SMDR record has 90 characters:

zmm/dd_hh:mmp_hh:mm:ss_pppp_fttt_xxxxxxxxxxxxxxxxxxxxxmmmmmhsqqqqk_rrrr_aaaaaaaaaaaasiii__

_________|_________|_________|_________|_________|_________|_________|_________|_________|

When "ANI/DNIS/ISDN/CLASS Number Delivery Reporting" is enabled in the SMDR Options form, the SMDR record is extended to 112 characters.

zmm/dd_hh:mmp_hh:mm:ss_pppp_fttt_xxxxxxxxxxxxxxxxxxxxxmmmmmhsqqqqk_rrrr_aaaaaaaaaaaasiii__

_________|_________|_________|_________|_________|_________|_________|_________|_________|

_aaaaaaaaaa_dddddddddd

_________|_________|__

When "Standardized Network OLI" is enabled in the SMDR Options form, the SMDR record is extended to 131 characters:

zmm/dd_hh:mmp_hh:mm:ss_pppp_fttt_xxxxxxxxxxxxxxxxxxxxxmmmmmhsqqqqk_rrrr_aaaaaaaaaaaasiii__

_________|_________|_________|_________|_________|_________|_________|_________|_________|

_aaaaaaaaaa_dddddddddd_psssccccs_pssscccc

_________|_________|_________|_________|_

Name | Columns | Symbol | Format | Definition | Notes
Long Call (call length) | 1 | z | (blank) | less than 5 mn |
- | from 5:00 to 9:59 mn
% | from 10:00 to 29:59 mn
+ | 30 mn or more
Date | 2 - 6 | mm/dd | mm | month (01-12) |
dd | day (01-31)
Spacer | 7 | _ | (blank) | space |
Start Time | 8-13 | hh:mm:ss:p | hh | hour (00-12 or 00-23) |
mm | minutes (00-59)
p | 12-hour clock: blank (A.M.) or P (P.M.) 24-hour clock: blank
Spacer | 14 | _ | (blank) | space |
Duration of Call | 15-22 | hh:mm:ss | hh | hour (00-99) | Maximum recorded time is 99:59:59.
mm | minutes (00-59)
ss | seconds (00-59)
Spacer | 23 | _ | (blank) | space |
Calling Party | 24-27 | pppp | cccc | extension number (0-9999) | Extension number can also contain * and #.
ATTm or ATmm | attendant console number (0-9 or 10-99)
Tnnn | CO trunk number (000-999)
Xnnn | non-CO trunk number (000-999)
Spacer | 28 | _ | (blank) | space |
Attendant | 29 | f | * | attendant involved | Attendant answered or initiated the call, then transferred it to an extension.
(blank) | attendant not involved
Time to Answer | 30-32 | ttt | ttt | time to answer in seconds (000 to 999) | Applies to incoming calls only.
*** | call unanswered
Spacer | 33 | _ | (blank) | space |
Digits Dialed on the Trunk | 34-59 or 34-54 | xxx...xxx | xx..xxyyyyy | x...x: Node ID + extension number (14 digits maximum) yyyyy: actual digits dialed T: network call | 26 digits maximum (20 is Meter Pulses enabled). If number of digits dialed exceeds space, remaining digits are not shown.
Tx..xxyyyyy
Meter Pulses | 55-59 | mmmmm | mmmmm | number of reversals received from outgoing trunk (00000 to 64000) | Optional. If not enabled, digits are used for Digits Dialed on the Trunk field.
Call Completion Status | 60 | h | A | answer supervision (outgoing) |
B | called party busy (incoming)
E | caller error (incoming)
T | Toll-denied (outgoing), TAFAS-answered (incoming) or pickup-answered (incoming)
I | internal call
Speed Call/Call Forward Flag | 61 | s | S | system or personal speed call | For forwarded internal calls, Third Party field is blank.
F | external call forwarded using External Call Forward or internal call forwarded using Call Forward
Called Party | 62-65 | qqqq | cccc | extension number (0-9999) | Extension numbers can also contain # and *. IP trunks are identified by X999.
Tnnn | CO trunk number (000-999)
Xnnn | non-CO trunk number (000-999)
ATTm or ATmm | attendant (0-9 or 10-99)
Transfer/Conference Flag | 66 | k | T | supervised transfer | Caller requeue (indicated by an "R" in the SMDR record) applies to calls to logged out ACD agents. For more information, see ACD and SMDR Reports.
X | unsupervised transfer
C | 3-way call or conference call
U | path unavailable (ACD)
I | interflow (ACD)
R | caller requeue
Spacer | 67 | _ | (blank) | space |
Third Party | 68-71 | rrrr | cccc | extension number (0-9999) | Can also contain # and *.
Spacer | 72 | _ | (blank) | space |
Account Code/Tag Call Identifier | 73-84 | aa...aa | aa...aa | account code number (2-12 digits, 00-99...99) or Tag Call Identifier (2 to 12 digits, a = 0-9, a-z, # or *) | Optional. NOTE: Some third-party SMDR log readers can only handle numeric characters in this field.
Route Optimization Flag | 85 | s | r | pre-optimization trunk | Applies to MSDN/DPNSS only.
R | post-optimization trunk
(blank) | no route optimization
System Identifier | 86-88 | iii | iii | System ID or Node ID (001-999, 000 if system and node ID not programmed) | When both System and Node ID are programmed, field displays System ID.
Spacer | 89 | _ | (blank) | space |
MLPP Precedence Level | 90 | j | 0 | Flash Override | Shows call precedence level for preemption. MLPP is not supported by the MiVoice Business System.
1 | Flash
2 | Immediate
3 | Priority
4 | Routine
With ANI/DNIS/ISDN/CLASS Number Delivery Reporting enabled:
Spacer | 91 | _ | (blank) | space |
ANI | 92-101 | aa...aa | aa...aa | ANI number (1-10 characters, 0-99...99) |
Spacer | 102 | _ | (blank) | space |
DNIS | 103-112 | dd...dd | dd...dd | DNIS number (1-10 characters, 0-99...99) |
With Standardized Network OLI enabled:
Spacer | 113 | _ | (blank) | space |
Call Identifier | 114-121 | pssscccc | p | plane (A-Z, odd letters for plane A, even letters for plane B) |
sss | system identifier (000-999)
cccc | call number (0000-9999)
Call Sequence Identifier | 122 | s | s | call sequence identifier (A-Z) | Does not rollover.
Spacer | 123 | _ | (blank) | space |
Associated Call Identifier | 124-131 | pssscccc | p | plane (A-Z, odd letters for plane A, even letters for plane B) |
sss | system identifier (000-999)
cccc | call number (0000-9999)

## Extended Digit Length SMDR Record Fields

The table below provides an overview of SMDR fields when "Extended Digit Length" is enabled in the SMDR Options form.

The Extended Digit Length SMDR record has 101 characters:

zmm/dd_hh:mmp_hhhh:mm:ss_ppppppp_fttt_xxxxxxxxxxxxxxxxxxxxxmmmmmhsqqqqqqqk_rrrrrrr_

_________|_________|_________|_________|_________|_________|_________|_________|___

aaaaaaaaaaaasiii__

______|_________|__

When "ANI/DNIS/ISDN/CLASS Number Delivery Reporting" is enabled in the SMDR Options form, the SMDR record is extended to 120 characters:

zmm/dd_hh:mmp_hhhh:mm:ss_ppppppp_fttt_xxxxxxxxxxxxxxxxxxxxxmmmmmhsqqqqqqqk_rrrrrrr_

_________|_________|_________|_________|_________|_________|_________|_________|___

aaaaaaaaaaaasiii___aaaaaaaaaa_ddddddd

______|_________|_________|_________|

When "Standardized Network OLI" is enabled in the SMDR Options form, the SMDR record is extended to 139 characters:

zmm/dd_hh:mmp_hhhh:mm:ss_ppppppp_fttt_xxxxxxxxxxxxxxxxxxxxxmmmmmhsqqqqqqqk_rrrrrrr_

_________|_________|_________|_________|_________|_________|_________|_________|___

aaaaaaaaaaaasiii___aaaaaaaaaa_ddddddd_psssccccs_pssscccc

______|_________|_________|_________|_________|_________|

Name | Columns | Symbol | Format | Definition | Notes
Long Call (call length) | 1 | z | (blank) | less than 5 mn |
- | from 5:00 to 9:59 mn
% | from 10:00 to 29:59 mn
+ | 30 mn or more
Date | 2 - 6 | mm/dd | mm | month (01-12) |
dd | day (01-31)
Spacer | 7 | _ | (blank) | space |
Start Time | 8-13 | hh:mm:p | hh | hour (00-12 or 00-23) |
mm | minutes (00-59)
p | 12-hour clock: blank (A.M.) or P (P.M.) 24-hour clock: blank
Spacer | 14 | _ | (blank) | space |
Duration of Call | 15-24 | hhhh:mm:ss | hhhh | hour (0000-9999) | Maximum recorded time is 9999:59:59.
mm | minutes (00-59)
ss | seconds (00-59)
Spacer | 25 | _ | (blank) | space |
Calling Party | 26-32 | ppppppp | ccccccc | extension number (0-9999999) | Extension number can also contain * and #.
ATTmm | attendant console number (00-99)
Tnnnn | CO trunk number (0-9999)
Xnnnn | non-CO trunk number (0-9999)
Spacer | 33 | _ | (blank) | space |
Attendant | 34 | f | * | attendant involved | Attendant answered or initiated the call, then transferred it to an extension.
(blank) | attendant not involved
Time to Answer | 35-37 | ttt | ttt | time to answer in seconds (0000 to 9999) | Applies to incoming calls only.
*** | call unanswered
Spacer | 38 | _ | (blank) | space |
Digits Dialed on the Trunk | 39-61 or 39-58 | xxx...xxx | xx..xxyyyyy | x...x: Node ID + extension number (14 digits maximum) yyyyy: actual digits dialed T: network call | 26 digits maximum (20 is Meter Pulses enabled). If number of digits dialed exceeds space, remaining digits are not shown.
Tx..xxyyyyy
Meter Pulses | 60-64 | mmmmm | mmmmm | number of reversals received from outgoing trunk (00000 to 64000) | Optional. If not enabled, digits are used for Digits Dialed on the Trunk field.
Call Completion Status | 65 | h | A | answer supervision (outgoing) |
B | called party busy (incoming)
E | caller error (incoming)
T | Toll-denied (outgoing), TAFAS-answered (incoming) or pickup-answered (incoming)
I | internal call
Speed Call/Call Forward Flag | 66 | s | S | system or personal speed call | For forwarded internal calls, Third Party field is blank.
F | external call forwarded using External Call Forward or internal call forwarded using Call Forward
Called Party | 67-73 | qqqqqqq | ccccccc | extension number (0-9999999) | Extension numbers can also contain # and *. IP trunks are identified by X9999.
Tnnnn | CO trunk number (0000-9999)
Xnnnn | non-CO trunk number (0000-9999)
ATTmm | attendant (00-99)
Transfer/ Conference Flag | 74 | k | T | supervised transfer |
X | unsupervised transfer
C | 3-way call or conference call
U | path unavailable (ACD)
I | interflow (ACD)
Spacer | 75 | _ | (blank) | space |
Third Party | 76-82 | rrrrrrr | ccccccc | extension number (0-9999999) | Can also contain # and *.
Spacer | 83 | _ | (blank) | space |
Account Code | 84-95 | aa...aa | aa...aa | account code number (2-12 digits, 00-99...99) or Tag Call Identifier (2 to 12 digits, a = 0-9, a-z, # or *) | Optional. NOTE: Some third-party SMDR log readers can only handle numeric characters in this field.
Route Optimization Flag | 96 | s | r | pre-optimization trunk | Applies to MSDN/DPNSS only.
R | post-optimization trunk
(blank) | no route optimization
System Identifier | 97-99 | iii | iii | System ID or Node ID (001-999, 000 if system and node ID not programmed) | When both System and Node ID are programmed, field displays System ID.
Spacers | 100 | _ | (blank) | space |
MLPP Precedence Level | 101 | j | 0 | Flash Override | Shows call precedence level for preemption MLPP is not supported by the MiVoice Business system.
1 | Flash |
2 | Immediate |
3 | Priority |
4 | Routine |
With ANI/DNIS/ISDN/CLASS Number Delivery Reporting enabled:
Spacer | 102 | _ | (blank) | space |
ANI | 103-112 | aa...aa | aa...aa | ANI number (1-10 characters, 0-99...99) |
Spacer | 113 | _ | (blank) | space |
DNIS | 114-120 | dd...dd | dd...dd | DNIS number (1-7 characters, 0-9999999) | Only 7 rightmost characters are recorded.
With Standardized Network OLI enabled:
Spacer | 121 | _ | (blank) | space |
Call Identifier | 122-129 | pssscccc | p | plane (A-Z, odd letters for plane A, even letters for plane B) |
sss | system identifier (000-999)
cccc | call number (0000-9999)
Call Sequence Identifier | 130 | s | s | call sequence identifier (A-Z) | Does not rollover.
Spacer | 131 | _ | (blank) | space |
Associated Call Identifier | 132-139 | pssscccc | p | plane (A-Z, odd letters for plane A, even letters for plane B) |
sss | system identifier (000-999)
cccc | call number (0000-9999)

## Extended Time to Answer SMDR Record Fields

When the "Extended Time to Answer" field is enabled in the SMDR Options form, the Time to Answer field is increased by one digit, and the spacer between the Calling Party and Attendant fields disappears.

The tables below show the changes to the SMDR fields when Extended Time to Answer is enabled. The changes are shown in bold. The same changes apply when ANI/DNIS/ISDN/CLASS Number Delivery Reporting and/or Standardized Network OLI are enabled.

### Standard SMDR Record fields with Extended Time to Answer Enabled

The Standard SMDR record with Extended Time to Answer enabled has 90 characters:

zmm/dd_hh:mmp_hh:mm:ss_ppppftttt_xxxxxxxxxxxxxxxxxxxxxmmmmmhsqqqqk_rrrr_aaaaaaaaaaaasiii__

_________|_________|_________|_________|_________|_________|_________|_________|_________|

Name | Columns | Symbol | Format | Definition | Notes
Calling Party | 27-30 | pppp | cccc | extension number (0-9999) | Extension number can also contain * and #.
ATTm or ATmm | attendant console number (0-9 or 10-99)
Tnnn | CO trunk number (000-999)
Xnnn | non-CO trunk number (000-999)
Attendant | 31 | f | * | attendant involved | Attendant answered or initiated the call, then transferred it to an extension.
(blank) | attendant not involved
Time to Answer | 32-35 | tttt | tttt | time to answer in seconds (0000 to 9999) | Applies to incoming calls only.
**** | call unanswered
Spacer | 36 | _ | (blank) | space |

### Extended Digit Length SMDR Record fields with Extended Time to Answer Enabled

The Extended Time to Answer SMDR with Extended Digit Length enabled record has 101 characters:

zmm/dd_hh:mmp_hhhh:mm:ss_pppppppftttt_xxxxxxxxxxxxxxxxxxxxxmmmmmhsqqqqqqqk_rrrrrrr_

_________|_________|_________|_________|_________|_________|_________|_________|___

aaaaaaaaaaaasiii__

______|_________|__

Name | Columns | Symbol | Format | Definition | Notes
Calling Party | 29-35 | ppppppp | ccccccc | extension number (0-9999999) | Extension number can also contain * and #.
ATTmm | attendant console number (00-99)
Tnnnn | CO trunk number (0-9999)
Xnnnn | non-CO trunk number (0-9999)
Attendant | 36 | f | * | attendant involved | Attendant answered or initiated the call, then transferred it to an extension.
(blank) | attendant not involved
Time to Answer | 37-40 | tttt | tttt | time to answer in seconds (0000 to 9999) | Applies to incoming calls only.
**** | call unanswered
Spacer | 41 | _ | (blank) | space |

## Extended Reporting Level 1 SMDR Record Fields

If "SMDR Extended Reporting Level 1" is enabled in the SMDR Options form, the ANI and DNIS field sizes are increased, and two new fields are added: LDN Called (after the Called Party field) and Suite Identifier (after the DNIS field). The changes are shown in the tables below (only the affected fields are shown).

The table below shows the changes to the SMDR fields when Extended Time to Answer is enabled. The changes are shown in bold.

NOTE: When Extended Reporting Level 1 is enabled, Extended Digit Length, Extended Time to Answer and Standardized Network OLI must also be enabled.

The Extended Report Level 1 SMDR record has 162 characters:

zmm/dd_hh:mmp_hhhh:mm:ss_pppppppftttt_xxxxxxxxxxxxxxxxxxxxxmmmmmhsqqqqqqq_lllllllk_rrrrrrr_

_________|_________|_________|_________|_________|_________|_________|_________|_________|_

aaaaaaaaaaaasiii___aaaaaaaaaaaaaaaaaaaa_dddddddddd_sssssss_psssccccs_pssscccc

________|_________|_________|_________|_________|_________|_________|_________|

Name | Columns | Symbol | Format | Definition | Notes
Called Party | 67-73 | qqqqqqq | ccccccc | extension number (0-9999999) | Extension numbers can also contain # and *. IP trunks are identified by X9999.
Tnnnn | CO trunk number (0000-9999)
Xnnnn | non-CO trunk number (0000-9999)
ATTmm | attendant (00-99)
Spacer | 74 | _ | (blank) | space |
LDN Called | 75-81 | lllllll | lllllll | extension number of attendant-answered call |
Transfer/ Conference Flag | 82 | k | T | supervised transfer |
X | unsupervised transfer
C | 3-way call or conference call
U | path unavailable (ACD)
I | interflow (ACD)
Spacer | 83 | _ | (blank) | space |
Third Party | 84-90 | rrrrrrr | ccccccc | extension number (0-9999999) | Can also contain # and *.
Spacer | 91 | _ | (blank) | space |
Account Code | 92-103 | aa...aa | aa...aa | account code number (2-12 digits, 00-99...99) or Tag Call Identifier (2 to 12 digits, a = 0-9, a-z, # or *) | Optional. NOTE: Some third-party SMDR log readers can only handle numeric characters in this field.
Route Optimization Flag | 104 | s | r | pre-optimization trunk | Applies to MSDN/DPNSS only.
R | post-optimization trunk
(blank) | no route optimization
System Identifier | 105-107 | iii | iii | System ID or Node ID (001-999, 000 if system and node ID not programmed) | When both System and Node ID are programmed, field displays System ID.
Spacer | 108 | _ | (blank) | space |
Autovon Call Priority Level | 109 | a | a | Autovon call priority level | Autovon is not used in 3300 ICP Release 8.0 or later.
Spacer | 110 | _ | (blank) | space |
ANI | 111-130 | aa...aa | aa...aa | ANI number (1-20 characters, 0-99...99) |
Spacer | 131 | _ | (blank) | space |
DNIS | 132-141 | dd...dd | dd...dd | DNIS number (1-10 characters, 0-99...99) |
Spacer | 142 | _ | (blank) | space |
Suite Identifier | 143-149 | sssssss | sssssss | suite identifier |
Spacer | 150 | _ | (blank) | space |
Call Identifier | 151-158 | pssscccc | p | plane (A-Z, odd letters for plane A, even letters for plane B) |
sss | system identifier (000-999)
cccc | call number (0000-9999)
Spacer | 159 | _ | (blank) | space |
Call Sequence Identifier | 160 | s | s | call sequence identifier (A-Z) | Does not rollover.
Spacer | 161 | _ | (blank) | space |
Associated Call Identifier | 162-169 | pssscccc | p | plane (A-Z, odd letters for plane A, even letters for plane B) |
sss | system identifier (000-999) |
cccc | call number (0000-9999) |

## Extended Reporting Level 1 and Level 2 SMDR Record Fields

If SMDR Extended Reporting Level 1 and Level 2 are enabled in the SMDR Options form, the Start Time field records the call start time to the second (hour:minute:second). Three new fields are added at the end: one for Two B-Channel Transfer Recording information and two for External Hot Desk User information.

The Extended Report Level 2 SMDR record has 195 characters:

zmm/dd_hh:mmp_hhhh:mm:ss_pppppppftttt_xxxxxxxxxxxxxxxxxxxxxmmmmmhsqqqqqqq_lllllllk_rrrrrrr_

_________|_________|_________|_________|_________|_________|_________|_________|_________|_

aaaaaaaaaaaasiii___aaaaaaaaaaaaaaaaaaaa_dddddddddd_sssssss_psssccccs_pssscccc

________|_________|_________|_________|_________|_________|_________|_________|

ttttt_eeeeeee_fffffff

________|_________|

Name | Columns | Symbol | Format | Definition | Notes
Called Party | 70-76 | qqqqqqq | ccccccc | extension number (0-9999999) | Extension numbers can also contain # and *. IP trunks are identified by X9999.
Tnnnn | CO trunk number (0000-9999)
Xnnnn | non-CO trunk number (0000-9999)
ATTmm | attendant (00-99)
Spacer | 77 | _ | (blank) | space |
LDN Called | 78-84 | lllllll | lllllll | extension number of attendant-answered call |
Transfer/ Conference Flag | 85 | k | T | supervised transfer |
X | unsupervised transfer
C | 3-way call or conference call
U | path unavailable (ACD)
I | interflow (ACD)
Spacer | 86 | _ | (blank) | space |
Third Party | 87-93 | rrrrrrr | ccccccc | extension number (0-9999999) | Can also contain # and *.
Spacer | 94 | _ | (blank) | space |
Account Code | 95-106 | aa...aa | aa...aa | account code number (2-12 digits, 00-99...99) or Tag Call Identifier (2 to 12 digits, a = 0-9, a-z, # or *) | Optional. NOTE: Some third-party SMDR log readers can only handle numeric characters in this field.
Route Optimization Flag | 107 | s | r | pre-optimization trunk | Applies to MSDN/DPNSS only.
R | post-optimization trunk
(blank) | no route optimization
System Identifier | 108-110 | iii | iii | System ID or Node ID (001-999, 000 if system and node ID not programmed) | When both System and Node ID are programmed, field displays System ID.
Spacer | 111 | _ | (blank) | space |
Autovon Call Priority Leve | 112 | a | a | Autovon call priority level | Autovon is not used in 3300 ICP Release 8.0 or later.
Spacer | 113 | _ | (blank) | space |
ANI | 114-133 | aa...aa | aa...aa | ANI number (1-20 characters, 0-99...99) |
Spacer | 134 | _ | (blank) | space |
DNIS | 135-144 | dd...dd | dd...dd | DNIS number (1-10 characters, 0-99...99) |
Spacer | 145 | _ | (blank) | space |
Suite Identifier | 146-152 | sssssss | sssssss | suite identifier |
Spacer | 153 | _ | (blank) | space |
Call Identifier | 154-161 | pssscccc | p | plane (A-Z, odd letters for plane A, even letters for plane B) |
sss | system identifier (000-999)
cccc | call number (0000-9999)
Spacer | 162 | _ | (blank) | space |
Call Sequence Identifier | 163 | s | s | call sequence identifier (A-Z) | Does not rollover.
Spacer | 164 | _ | (blank) | space |
Associated Call Identifier | 165-173 | pssscccc | p | plane (A-Z, odd letters for plane A, even letters for plane B) |
sss | system identifier (000-999)
cccc | call number (0000-9999)
Two B-Channel Transfer Recording | 174-179 | tttttt | tttttt | tag ID provided by the CO |
Spacer | 180 | _ | (blank) | space |
Calling External Hot Desk User | 181-187 | eeeeeee | ccccccc | extension number (0-9999999) |
Called External Hot Desk User | 189-195 | fffffff | ccccccc | extension number (0-9999999) |
Spacer | 196 | _ | (blank) | space |
Calling Party Location Identifier | 197-201 |  |  | The location identifier for the calling party. A 5 ASCII character string. | The Location Identifier fields apply to consoles and sets only, not trunks.
Spacer | 202 | _ | (blank) |  |
Called Party Location Identifier | 203-207 |  |  | The location identifier for the called party. A 5 ASCII character string. | The Location Identifier fields apply to consoles and sets only, not trunks.

Related Topics

- SMDR Extended Reporting

- SMDR Examples