# MONITOR DISPLAY

## Qualifiers:

None

## Purpose:

Use this command to list the monitors established by a particular host command interface (HCI) session.

## Details:

Field Name | Description
Mon | Device monitor identification number.
LID | PABX software identifier of the monitored device.
DN | Directory number of the monitored device.
State | Current call state reported to the host application program.
Msgs | The number of call status messages sent to the host by the PABX.
CP Card | Physical location of the communications processor from which the monitor was set.
Totals - monitors | The total number of devices being monitored.
Totals - call statuses | The total number of call status messages sent to the host for all currently active monitors.

## Example:

### Entry: MONITOR DISPLAY

System Response:

Displaying all monitors on main control.

Mon LID DN State Msgs CP Card
Cab Shlf Slot Cir

1 7D000002 5555 unavailabl 0 01 01 10 01

Totals - monitors: 1 - call statuses: 0.