# Programming 5240 IP Phones

## Before You Begin

- If you wish to program a MiVoice IP Phone with a static IP address, refer to the Technician's Handbook.

- Ensure the DHCP Server has been programmed.

- Enter IP user licenses in the License and Option Selection form.

- Specify IP Telephone Set Registration Access Code, Set Replacement Access Code, and Set Registration Security Code in the System Options form.

- Program Class of Service, Interconnect Restriction, and Intercept Handling for each device.

NOTE: The Class of Service must have both the HCI/CTI/TAPI Call Control Allowed option, and the HCI/CTI/TAPI Monitor Allowed option enabled.

## Programming

To program IP Phones:

1. Multiline IP Sets form

- Complete the Device Type, Prime Directory Number, Prime Line Type, Interconnect Number, and the MAC address (optional) fields.

2. (Optional) Multiline Set Keys form

- Assign a directory number (line appearance) or feature to each key.

- Assign each line appearance a ring type.

3. (Optional) Multiline Appearance Groups form

- Change the ring type at each telephone where this number appears.

- Change the group type from "key system" to "multicall" or vice versa.

4. (Optional) Default Account Codes form

- Create a default account code number that will appear in all SMDR records for the station.

5. Station Attributes form

- Assign a Class of Service, Class of Restriction, and Intercept Number to the directory number of the telephone.

- (Optional) Assign a Default Account Code Index number.

6. User and Services Configuration form

- Use the User and Services Configuration search field to locate the directory number that you assigned to the device. Assign a name, department, and location to the directory number.

7. (Optional) Register the IP telephone.

- This step is required only if the MAC address was not programmed in the Multiline IP Sets form.

NOTE: If you delete telephones, you must also delete the corresponding directory entries and voice mailboxes.