# Maintenance Commands

A | B | C | D | E | F | G | H | I | J | K | L | M
N | O | P | Q | R | S | T | U | V | W | X | Y | Z

### ALARMS

### ARPSHOW

### BLF ALLOW LOGS

### BLF FILTER LOGS

### BLF LOGS STATUS

### BLF REFRESH

BLF REFRESH CEID <CEID INDEX>

BLF REFRESH CEID ALL

### BLOCKED_CALLS

BLOCKED_CALLS SHOW

BLOCKED_CALLS CLEAR

### BRI

BRI CONFIGURATION MMC ALL

BRI CONFIGURATION MMC <number>

### BUSY

BUSY <cabinet> <shelf> <slot>

BUSY <cabinet> <shelf> <slot> <circuit>

BUSY <cabinet> <shelf> <slot> <circuit> <hybrid>

BUSY EXTENSION <extension number>

BUSY RESET <number>

BUSY TRUNK GROUP <group number>

BUSY XNET ALL

BUSY XNET ALL IP

BUSY XNET ALL ISDN

BUSY XNET ICP <ICP number>

BUSY XNET ICP <ICP number> IP

BUSY XNET ICP <ICP number> ISDN

### BWM STATISTICS RESET

### CALLING PARTY PAYS

calling_party_pays display

calling_party_pays rebuild_tree

calling_party_pays find <dn>

### CANCEL PRINT

CANCEL PRINT ALL

CANCEL PRINT ALL /PORT <port name>

CANCEL PRINT /PORT <port name>

CANCEL PRINT <job number>

CANCEL PRINT <job number> /PORT <port name>

### CATALOG INFO

CATALOG INFORMATION <path name>

CATALOG INFORMATION <path name> FULL

CATALOG INFORMATION <path name> SUBCATALOGS

CATALOG INFORMATION <path name> TOTAL

### CBM

CBM DISABLE LOG

CBM ENABLE LOG

### CCS

CCS RESET DASS2

CCS RESET DPNSS ROUTE_OPT_STATISTICS

CCS SHOW DASS2 FEATURE_STATUS

CCS SHOW DASS2 ROUTE_OPT_STATISTICS

CCS SHOW DPNSS

CCS TRACE CLEAR CONTEXT

CCS TRACE DISABLE

CCS TRACE ENABLE

CCS TRACE ENABLE CONTINUOUS

CCS TRACE SET CONTEXT <location ID>

CCS TRACE SET CONTEXT VIRTUAL <location ID>

CCS TRACE SET CONTEXT XNET

CCS TRACE SHOW CONTEXT

CCS TRACE SHOW OUTPUT

### CONGESTION

### CP SERVICE

CP SERVICE DAY

CP SERVICE DISPLAY

CP SERVICE NIGHT1

CP SERVICE NIGHT2

### CRS PURGE

CRS PURGE EMERGENCY_DID

### CRS QUERY

CRS QUERY ALLOW_LIST

CRS QUERY DENY_LIST

CRS QUERY EMERGENCY_DID <digit string>

### CRS SHOW

CRS SHOW EHDU

CRS SHOW EMERGENCY_DID

CRS SHOW DID

CRS SHOW ALL

CRS SHOW <DN digit string>

CRS SHOW ALLOW_LIST

CRS SHOW DENY_LIST

### DATABASE AUDIT

### DBMS

DBMS CHECK BRIEF

DBMS CHECK FULL

DBMS CHECK KILL

DBMS CHECK ON

DBMS CHECK OFF

DBMS CHECK TIME <hour>

DBMS CLIENT

DBMS FLAG OFF

DBMS SAVE

DBMS STATUS

### DBTAB

DBTAB <table id>

DBTAB <table id> <record id>

### DGT TRACE

DGT AT <digit string>

DGT TRACE <strparam1>

DGT TRACE <MMC Pilot Number>

DGT TRACE LBN <digit string 1> <digit string 2>

### DISK USAGE

### DISPLAY ASU INFO

### DTSTAT

DTSTAT CLEAR <unit> <shelf> <slot> <hybrid>

DTSTAT READ <unit> <shelf> <slot> <hybrid>

DTSTAT READ <unit> <shelf> <slot> <hybrid> LAST <number of hours>

### DNS

DNS SHOW

DNS CLEAR

### DUMPDSPBOOTINFO

### EDT

EDT CANCEL HANDOFF

EDT COURTESY HANDOFF

EDT DELETE

EDT DISABLE

EDT Enable

EDT FORCE FAILBACK

EDT FORCE FAILOVER

EDT HELP

EDT SHOW

EDT SHOW RESILIENCY

EDT TRACE

###

### GDM CHECK USERANDSERVICE

### GDM REPAIR USERANDSERVICE

### HANDOFFSERVICE SHELL COMMANDS

hsHelp

hsShowIcps

hsShowSets

hsHandoff

hsHandback

hsPushback

hsDebug

hsTrace

### HANDOFF SERVICES TYPE COMMANDS

HST COURTESY HANDOFF

HST CANCEL HANDOFF

HST STATUS HANDOFF

HST POLL HANDOFF

### HISTORY

HISTORY DELETE ALL

HISTORY DELETE [EXT yyyy] | ALL

### HTMLAPPUPGRADE

### I (INFORMATION)

### INETSTATSHOW

### L2 POESTATUS

### L2 STAT MACLIST

L2 STAT MACLIST <port_number>

### L2 STAT PORT

L2 STAT PORT <port_number>

### L2 STAT SPANNING TREE

### L2 STAT SWITCH

NOTE: Layer 2 commands are not applicable to MiVoice Business for Industry Standard Servers (ISS) since Layer 2 switching is performed by an external Layer 2 switch.

### LANGUAGE ADD

LANGUAGE ADD <language> SETS DEFAULT FROM *.LANGSEL

LANGUAGE ADD <language> SETS AUX1 FROM *.LANGSEL

LANGUAGE ADD <language> SETS AUX2 FROM *.LANGSEL

### LANGUAGE DISPLAY

LANGUAGE DISPLAY SETS DEFAULT

LANGUAGE DISPLAY SETS AUX1

LANGUAGE DISPLAY SETS AUX2

### LANGUAGE SELECT

LANGUAGE SELECT <language> SETS DEFAULT FROM *.LANGSEL

LANGUAGE SELECT <language> SETS AUX1 FROM *.LANGSEL

LANGUAGE SELECT <language> SETS AUX2 FROM *.LANGSEL

### LGMR SHOW

LGMR SHOW CGPN <ANI>

LGMR SHOW GROUP <GroupDN>

LGMR SHOW MEMBER <MemberDN>

LGMR SHOW TOTALS

### LICENSE STATUS

### LOAD

LOAD <unit/module>

LOAD IPDevice <1,2...700>

LOAD IPDevice <1> TO <700>

LOAD CONTROLLER

### LOCATE

LOCATE AGENT <agent identifier>

LOCATE ALL FREE DN <dnmin> TO <dnmax>

LOCATE ALL FREE PLID <card type> <unit>

LOCATE ALL FREE PLID <card type> <unit> <shelf>

LOCATE ALL FREE PLID <card type> <unit> <shelf> <slot>

LOCATE ALL FREE PLID <card type> <unit> <shelf> <slot> <circuit>

LOCATE ALL FREE PLID <card type> <unitmin> TO <unitmax>

LOCATE AUTO_DN

LOCATE EXTENSION <extension number>

LOCATE FEATURE EXT <extension number>

LOCATE FEATURE HUNT_GROUP <number>

LOCATE FEATURE PLID <unit> <shelf> <slot>

LOCATE FEATURE PLID <unit> <shelf> <slot> <circuit>

LOCATE FIRST FREE DN <dnmin> TO <dnmax>

LOCATE FIRST FREE PLID <card type> <unit>

LOCATE FIRST FREE PLID <card type> <unit> <shelf>

LOCATE FIRST FREE PLID <card type> <unit> <shelf> <slot>

LOCATE FIRST FREE PLID <card type> <unit> <shelf> <slot> <circuit>

LOCATE FIRST FREE PLID <card type> <unitmin> TO <unitmax>

LOCATE GROUP_REPORTING_NUM <number>

LOCATE HOT_DESK_USER ALL

LOCATE HOT_DESK_USER TARGETS

LOCATE HOT_DESK_USER ACTIVE

LOCATE HOT_DESK_USER INACTIVE

LOCATE LICENSE

LOCATE NUMBER <number>

LOCATE MOBILE_DN ALL

LOCATE MOBILE_DN TARGETS

LOCATE MOBILE_DN ACTIVE

LOCATE MOBILE_DN INACTIVE

LOCATE OPERATORS

LOCATE PATH_REPORTING_NUM <number>

LOCATE PLID <unit> <shelf> <slot>

LOCATE PLID <unit> <shelf> <slot> <circuit>

LOCATE PLID <unit> <shelf> <slot> <circuit> <channel>

LOCATE REMOTE_DN <number>

LOCATE SERVICE LEVEL

LOCATE SERVICE LEVEL DEVICE_ONLY

LOCATE SERVICE LEVEL MULTI_DEVICE

LOCATE SERVICE LEVEL PENDING_USER

LOCATE SERVICE LEVEL TRUSTED

LOCATE SERVICE LEVEL SUMMARY

LOCATE TENANT

LOCATE TENANT <number>

LOCATE TRUNK <trunk number>

### LOGOUT HOTDESK

LOGOUT HOTDESK ALL

LOGOUT HOTDESK EXTERNAL ALL

LOGOUT HOTDESK INTERNAL ALL

### LOGSYS

LOGSYS ATTRIBUTES <logname>

LOGSYS CANCEL P <logname>

LOGSYS PRINT <logname>

LOGSYS PRINT <logname> ALL

LOGSYS READ <logname> ALL

LOGSYS READ <logname> ALL MATCH <string>

LOGSYS READ <logname> INTO <filename> ALL

LOGSYS READ <logname> INTO <filename> ALL MATCH X

LOGSYS READ <logname> NEWEST X

LOGSYS READ <logname> NEWEST X MATCH <string>

LOGSYS READ <logname> INTO <filename> NEWEST X

LOGSYS READ <logname> INTO <filename> NEWEST X MATCH X

LOGSYS READ <logname> OLDEST X

LOGSYS READ <logname> INTO <filename> OLDEST X

LOGSYS READ <logname> INTO <filename> OLDEST X MATCH X

LOGSYS SIZE <logname> RAM <number of bytes>

LOGSYS SIZE <logname> FILE <entry count>

### MESSAGE

MESSAGE REMOTE

MESSAGE SUBSYSTEM

### MITAIDISPLAYMONSUMMARY

### MITAISHOWMONSTAT

### MONITOR DISPLAY

### MOVE SWAP

### NETSYNC

NETSYNC SETSOURCE <source number>

NETSYNC SETSOURCE AUTO

NETSYNC SETSOURCE FREERUN

NETSYNC STATE

NETSYNC SUMMARY <number>

NETSYNC SUMMARY <number> LAST <number of hours>

### PCM

PCM STATUS RX <link>

PCM STATUS TX <link>

PCM TOTALS

### PING

PING < IP_address | hostname>

PING < IP_address | hostname> < number_packets>

### PLATFORMTYPE

### PMS

PMS TRACE DISABLE

PMS TRACE ENABLE

PMS STATE

### PROGRAMMED FAILBACK (PROG F)

PROGRAMMED FAILBACK ON

PROGRAMMED FAILBACK OFF

PROGRAMMED FAILBACK DISPLAY

PROGRAMMED FAILBACK SCHEDULE <hh:mm:ss>

### PROGRAMMED REBOOT

PROGRAMMED REBOOT COURTESY ON

PROGRAMMED REBOOT COURTESY OFF

PROGRAMMED REBOOT DISPLAY

PROGRAMMED REBOOT RESOURCE RECOVERY ON

PROGRAMMED REBOOT RESOURCE RECOVERY OFF

PROGRAMMED REBOOT RESOURCE RECOVERY <hh:mm:ss>

PROGRAMMED REBOOT SCHEDULE ON

PROGRAMMED REBOOT SCHEDULE OFF

PROGRAMMED REBOOT SCHEDULE <DAILY> <hh:mm:ss>

PROGRAMMED REBOOT SCHEDULE <day-of-week> <hh:mm:ss>

PROGRAMMED REBOOT SCHEDULE MONTHLY <week # [1-4]> <day-of-week> <hh:mm:ss>

PROGRAMMED REBOOT SCHEDULE INTERVAL <interval in weeks [1-52]> <MMM> <day-of-month> <hh:mm:ss>

### PROGRAMMED SERVICE

PROGRAMMED SERVICE SCHEDULE NIGHT1 DAILY <hh:mm:ss>

PROGRAMMED SERVICE SCHEDULE NIGHT1 ON/OFF

PROGRAMMED SERVICE SCHEDULE NIGHT2 DAILY <hh:mm:ss>

PROGRAMMED SERVICE SCHEDULE NIGHT2 ON/OFF

PROGRAMMED SERVICE SCHEDULE DAY DAILY <hh:mm:ss>

PROGRAMMED SERVICE SCHEDULE DAY ON/OFF

PROGRAMMED SERVICE SCHEDULE ON/OFF

PROGRAMMED SERVICE DISPLAY

### PS

### READDATETIME

RECONCILE CLUSTER AND RDN

### REMOVEDLMDATA

### REMOVE COURTESY DOWN

REMOVE COURTESY DOWN <unit> <shelf> <slot> <circuit>

REMOVE COURTESY DOWN EXTENSION <extension number>

### REMOVENE

### REMOVESHARINGNE

### RENEWFWTABLES

### RESET

RESET SYSTEM

RESET IGW

RESET L2SWITCH

RESET MIPS

### RESOURCES

RESOURCE <unit> <shelf> <slot> <circuit or hybrid>

RESOURCE <unit> <shelf> <slot> <circuit or hybrid> <channel>

RESOURCE XNET <trunk>

### RESET_ALL_LOGIN_PASSWORDS

### RESET_LOGIN_PASSWORD

### RESTART CALLSERVER

### RETURN TO SERVICE

RTS <unit> <shelf> <slot>

RTS <unit> <shelf> <slot> <circuit or hybrid>

RTS <unit> <shelf> <slot> <circuit or hybrid> <channel>

RTS EXTENSION <extension number>

RTS TRUNK GROUP <group number>

RTS XNET ALL

RTS XNET ALL IP

RTS XNET ALL ISDN

RTS XNET ICP <ICP number>

RTS XNET ICP <ICP number> IP

RTS XNET ICP <ICP number> ISDN

### RMESSAGE

RMESS VERIFY PBX <pbx number> LAN

RMESS VERIFY PBX <pbx number> PPP

### ROUTESHOW

### SASTATS

SASTATS DISPLAY ALL

SASTATS DISPLAY CALLS

SASTATS DISPLAY FEATURES

SASTATS DISPLAY RESOURCES

SASTATS RESTART

### SCHEDULE

### SET

SET THRESHOLDS < alarm category> <minor threshold> <major threshold> <critical threshold>

### SET EX CONFIGURATION

SET EX CONFIGURATION

### SHOW EX CONFIGURATION

SHOW EX CONFIGURATION

SHOW EX CONFIGURATION HELP

### SHOW

SHOW FAULTS ALARMS

SHOW FAULTS <alarm category>

SHOW PRINT

SHOW PRINT <printer name>

SHOW PRINT ALL

SHOW STATUS <alarm category>

SHOW STATUS ALARMS

SHOW STATUS ALARMS ALL

### SHOWDSPSTATUS

### SHUTDOWN

SHUTDOWN

### SILOSHOWMAXFREE

### SIP

SIP BUSY FORCE PEER <PEER_NAME>

SIP BUSY PEER <PEER_NAME>

SIP CONFIGURATION

SIP DEBUG <ON/OFF><APP, AUX, MH, SSM, SSP>

SIP <COMP_ID> TRACE <TRACE_FLAG>

SIP <COMP_ID> SET LEVEL <TRACE_LEVEL>

SIP <COMP_ID> TAIL <TAIL_FLAG>

SIP DEBUG <ON/OFF><APP, AUX, MH, SSM, SSP>

SIP HELP

SIP LINK STATE ALL

SIP LINK STATE PEER <PEER_NAME>

SIP LINK STATUS

SIP REGISTRAR ALL

SIP REGISTRAR DECT

SIP REGISTRAR DEVCAP <N>

SIP REGISTRAR HOTDESK

SIP REGISTRAR ONSECONDARY

SIP REGISTRAR STATS

SIP REGISTRAR UA <SUB_STRING>

SIP REGISTRAR UCENDPOINT

SIP REREGISTER PEER <PEER_NAME>

SIP RTS PEER <PEER_NAME>

SIP SHOW ACTIVE ALL

SIP SHOW ACTIVE PEER <PEER_NAME>

SIP SHOW ACTIVE PROFILE <PROFILE_NAME>

SIP STATS BOTH

SIP STATS CLEAR

SIP STATS PROFILE <PROFILE_NAME>

SIP STATS TRUNKS

SIP TCPDUMP ON

SIP TCPDUMP OFF

### SIPDECT

SIPDECT CHECK <ACTION>

SIPDECT CREATE PROFILE

SIPDECT SYNC <ACTION>

### SIP TRAFFIC

SIP TRAFFIC XMLPRINT NEXT

SIP TRAFFIC XMLPRINT OLDEST

SIP TRAFFIC XMLPRINT NEWEST

SIP TRAFFIC PRINT NEXT

SIP TRAFFIC PRINT OLDEST

SIP TRAFFIC PRINT NEWEST

### SLOTALLINFO

### STATE

STATE <unit>

STATE <unit> <shelf>

STATE <unit> <shelf> <slot>

STATE <unit> <shelf> <slot> <circuit or hybrid>

STATE <unit> <shelf> <slot> <circuit or hybrid> <channel>

STATE EXTENSION <extension number>

STATE MLS <unit> <shelf> <slot> <circuit or hybrid>

STATE TRUNK GROUP <group number>

STATE TRUNK GROUP <group number> TRAFFIC

STATE TRUNK GROUP <group number> VIRTUAL

STATE TRUNK GROUP <group number> ALL

STATE XNET ICP <ICP number>

STATE XNET ALL

STATE XNET ALL IP

STATE XNET ALL ISDN

STATE XNET TRUNK <trunk number>

STATE XNET LINK <link number>

### SYSTEM TOTALS

### TRACERT

RTC <ip address> /HOPS n /WAIT n

IPSET <ip address> to <ip address> /HOPS n /WAIT n

### TRAFFIC

TRAFFIC DELETE <MMM - dd hh : mm>

TRAFFIC FILES

TRAFFIC PRINT <MMM - dd hh : mm>

TRAFFIC STATUS

TRAFFIC STOP

### TYPE

TYPE *.DR.LOGFILE_1

### UPGRADEBOOTROM

UPGRADEBOOTROM RTC

UPGRADEBOOTROM E2T

UPGRADEBOOTROM ALL

### UPTIME

### VERSION

VERSION

### VOICE MAIL

VOICE MAIL

### WHERE

WHERE