# Interconnect Restrictions

## Description

Each peripheral device is assigned an Interconnect Number that is used to restrict one device from connecting with another. Interconnect Restrictions can be used to restrict access to certain trunks, stations, or equipment (i.e. data communications equipment). The restriction is also a function of the direction of the call.

## Conditions and Feature Interactions

- Interconnect restrictions cannot be overridden by user features.

- If you attempt to violate an Interconnect Restriction, you will hear reorder tone or your call will be rerouted (see Intercept Handling).

## Programming

1. Assign an Interconnect Number to each station/circuit in that station's form (for example, the Analog Sets form )

2. Digital Trunks form

- Assign an Interconnect Number to each trunk in the

3. Interconnect Restriction form

- Assign restrictions to the Interconnect Numbers in the

## Device Support

Not applicable

## Operation

None

Related Topics

- Intercept Handling