# SHOWDSPSTATUS

## Qualifiers:

None

## Purpose:

Use this command to display the current status of all detected DSP MMCs on the system.

## Example:

### Entry: SHOWDSPSTATUS

System Response:

Dsp Status: (Warning! This only displays the current state of the dsps in the system.

Failures previous to a system reboot are not recorded.)

Slot Number 3 Dsp 0 State: ACTIVE

Slot Number 3 Dsp 1 State: ACTIVE

Slot Number 3 Dsp 2 State: ACTIVE

Slot Number 3 Dsp 3 State: ACTIVE

Slot Number 4 Dsp 0 State: ACTIVE

Slot Number 4 Dsp 1 State: ACTIVE

Slot Number 4 Dsp 2 State: ACTIVE

Slot Number 4 Dsp 3 State: ACTIVE

Slot Number 6 Dsp 0 State: ACTIVE

Slot Number 6 Dsp 1 State: ACTIVE

Slot Number 6 Dsp 2 State: ACTIVE

Slot Number 6 Dsp 3 State: ACTIVE