# DISPLAY ASU INFO

## Qualifiers:

None

## Purpose:

Displays the hardware version, status, and other information about the ASU (Embedded ASU, AMB, AOB, ASU, and ASU II) devices connected to the CIM ports on the MiVoice Business system.

## Details:

The command output is as follows:

- CIM: port number in the range 1 to 21. CIM 1 is always the Embedded ASU.

- STATUS: the CIM Port sync status— either UAPI_APH_UP if the ASU is plugged into the port or UAPI_APH_DOWN if it is not. For the Embedded ASU, it is always UAPI_APH_UP since the CIM 1 port is logical port.

- UAPI TYPE (HUBSP TYPE): the type (UAPI TYPE) and country variant (HUBSP TYPE) of ASUs installed. For external Universal and ONS ASUs, HUBSP TYPE indicates its hardware variant. For the Embedded ASU, ASU II, and AX the HUBSP TYPE is COMBO with the same country variant as the MiVoice Business system (as specified in the License and Option Selection form).

Type Codes (UAPI TYPE)
Code | Meaning
DS_HUBTYPE_NONE | No device installed
DS_COMBO | Universal ASU
DS_ONS | ONS ASU
DS_AMB_64 | Embedded ASU on CX II/MXe III
DS_AMB_AOB_64 | Embedded ASU on CX II/MXe III with AOB
DS_ASU_2G | ASU II
DS_PER_2G | AX

Country Variant Codes (HUBSP TYPE)
Code | Meaning
HUB_TYPE_NULL | No device installed
HUB_TYPE_NA_COMBO | North American Universal ASU
HUB_TYPE_NA_ONS | North American ONS ASU
HUB_TYPE_UK_COMBO | United Kingdom Universal ASU
HUB_TYPE_UK_ONS | United Kingdom ONS ASU
HUB_TYPE_LA_COMBO | Latin American Universal ASU
HUB_TYPE_LA_ONS | Latin American ONS ASU
HUB_TYPE_EU_COMBO | European Universal ASU
HUB_TYPE_EU_ONS | European ONS ASU

- CARD INFO: HEX values identifying the ASU cards by the type of circuits (ONS, LS trunk, Paging, Music On Hold) they support. The number of HEX values displayed is equal to the number of card slots (logical or physical) in the ASU. For example, the ASU II displays two values, one for each physical card slot. The embedded ASU has four values: three for circuits on the Embedded ASU and one (the second of the four) for the AOB.

Hex Value | Card Type
00 | No Card Installed
3D | 8 cct ONS. Used in Combo/ONS ASUs
3E | 4 LS trunk ccts. Used in Universal ASUs
21 | 4 MOH ccts. Used in Universal ASUs
53 | 2 Paging ccts. Used in Universal ASUs
51 | 1 MOH cct. Used in Embedded ASU of CX II
50 | 1 Paging cct. Used in Embedded ASU of CX II
55 | 4 ONS, 6 LS ccts. Used in Embedded ASU of CX II
57 | 16 ONS ccts. Used in ASU II and AX
58 | 12 ONS & 4_LS ccts. Used in ASU II and AX
5A | 24 ONSP ccts. Used in ASU II and AX

- Cim <port number> Prom: shows the Marketing Part Number (MPN), Circuit Card Assembly (CCA) number, and the hardware revision of the ASU. In the example below for CIM 1, the MPN is 50003724, the CCA is 56005264 and the hardware dot revision is B.04. If the AOB is installed, its PROM string will appear after the Embedded ASU string. A list of MPNs and the associated hardware is provided in the "FRU Part Number" section of the MiVoice Business Technician's Handbook.
  The AMB is only available for the CX II/CXi II, and MXe III controllers. The marketing part numbers for the AMBs are
  - 50005184 -- AMB v3 on on CXi II, MXe III
  For the ASU II, the MPN of the ASU II controller (50005105) is shown in the Prom string.
  For line cards the MPNs are as follows:
  - 50005103 -- 16 ONS port
  - 50005533 -- 16 ONS port protected
  - 50005104 -- 12 ONS and 4 Loop Start
  - 50005721 -- 24 ONS port
  - 50005731 -- 24 ONS port protected-
  The CCA identification numbers identify the versions of the AMB and ONS cards as listed below:
  - 56006404RB -- v1
  - 56007302RA -- v2
  - 56008261RA -- v2
  - 56008157RB -- v3

- FW: Firmware string showing the MAC address of the ASU, and the version/date tag for the BOOTROM and main firmware load.

NOTE: Cim Prom and Firmware strings are not provided for the AX controller since they are the same as the host MiVoice Business system.

## Example:

### Entry: DISPLAY ASU INFO

System Response:

CIM STATUS UAPI TYPE (HUBSP TYPE) CARD INFO
---------------------------------------------------------------------------
1 UAPI_APH_UP DS_AMB (NA COMBO) (4F 00 51 50)
2 UAPI_APH_UP DS_ASU2G (NA COMBO) (57 00)
3 UAPI_APH_UP DS_ONS (NA ONS) (3D 3D 3D)
Cim1 Prom: 50003724 56005264RB.04 08000F0075D5 1 132424232213
FW: MAC:08000F0075D5 | MAIN Ver:04.00.00.09 Date:Aug 22 2006 Time:16:31:
30 | FLASH = MAIN
Cim2 Prom: 50005105 56007252RA.04 08000F1AE020
FW: MAC:08000F1AE020 | MAIN Ver:01.00.00.16 Date:Sep 05 2006 Time:16:30:
06 | BOOT Ver: 01.00.00.01 Date:Oct 24 2005 Time:16:40:01
Cim3 Prom: 50001267 150359301RA 08000F008E6E 1 3A 192.168.010.001 192.168.010.001 /sysro/APH_Project.hex E9
FW: MAC:08000F008E6E | MAIN Ver:05.00.00.10 Date:Sep 05 2006 Time:16:50:
56 | FLASH Ver:05.00.00.10 Date:Sep 05 2006 Time:16:46
value = 1 = 0x1