# DUMPDSPBOOTINFO

## Qualifiers:

None

## Purpose:

Use this command to display DSP resource allocation on the system.

## Example:

### Entry: DUMPDSPBOOTINFO

### System Response:

Dsp(0,0): mmcSlot=1 (1-based) Load Type: TELEPHONY(1,"/sysro/DspConfig/TELEPHON) Mod Type: NOCONFERENCE(1) Dsp(1,0): mmcSlot=6 (1-based) Load Type: TELEPHONY(1,"/sysro/DspConfig/TELEPHON) Mod Type: NOCONFERENCE(1) Dsp(1,1): mmcSlot=6 (1-based) Load Type: TELEPHONY(1,"/sysro/DspConfig/TELEPHON) Mod Type: NOCONFERENCE(1) Dsp(1,2): mmcSlot=6 (1-based) Load Type: TRANSCODER(2,"/sysro/DspConfig/TRANSCO) Mod Type: DEFAULT(0) Dsp(1,3): mmcSlot=6 (1-based) Load Type: TELEPHONY(1,"/sysro/DspConfig/TELEPHON) Mod Type: NOCONFERENCE(1) Dsp(2,0): mmcSlot=7 (1-based) Load Type: ECHOCANCELLER(3,"/sysro/DspConfig/ECHO) Mod Type: DEFAULT(0) Dsp(2,1): mmcSlot=7 (1-based) Load Type: ECHOCANCELLER(3,"/sysro/DspConfig/ECHO) Mod Type: DEFAULT(0) Dsp(2,2): mmcSlot=7 (1-based) Load Type: TELEPHONY(1,"/sysro/DspConfig/TELEPHON) Mod Type: NOCONFERENCE(1) Dsp(2,3): mmcSlot=7 (1-based) Load Type: TELEPHONY(1,"/sysro/DspConfig/TELEPHON) Mod Type: DEFAULT(0)