# RESET E2T

## Qualifiers:

None

## Purpose:

Resets the E2T
Ethernet to TDM converter. Gateway between the traditional circuit-switched, time division multiplexed telephone systems and IP devices on the Ethernet. card in Expanded MXe systems.

NOTE: This command should be used only if the E2T card is not connected to the E2T proxy SP; otherwise, it triggers a system reset.

## Example:

### Entry: RESET E2T

### System Response:

please wait...
.. Reset E2T in progress...
.. Please allow two minutes to complete.