# Secure Call Indication

## Description

The Secure Call Indication is a feature by which MiVB sends an icon to be displayed on MiNET sets to indicate calls that are encrypted end-to end.

NOTE: MiVB sends the Secure Call Indication to all MiNET sets. Only MiNET sets that have the capability will display the icon.

## Conditions and Feature Interactions

- Secure Call Indication feature applies only for the 69xx devices.

- Secure call indication is NOT sent to the MiNET set if the call is not encrypted or when the call is encrypted, but is among the following:

- - Calls on a SIP trunk

  - Calls on an TDM Trunk

  - Calls on an analogue trunk

  - Conference calls hosted on the MiVB or AWV

  - Calls on which Music on Hold is enabled

  - Calls that are on Recorded Announcement Device

  - Calls on a voice mail port on the MiVB or NuPoint

  - Calls that are being recorded via the Record A Call feature

  - Calls that are being monitored by an agent

## Programming

- Ensure that the system Options - Voice Encryption Enabled and Voice/Video SRTP Encryption Enabled are set to Yes.

## Operation

None