# IP/XNET Trunk Profiles

## Purpose

The IP/XNET Trunk Profiles form is used to program trunk service or interconnect restriction parameters specific to IP Networking or XNET.

Use this form when performing the following tasks:

- IP Networking/XNET Planning

- IP Networking Programming

- XNET Programming

- see an XNET Programming Example

For more information:

- IP Networking/XNET Description

## Field Descriptions

Parameter | Description | Default Value
Local Profile Number | System-generated, protected field. Identifies each profile. |
Trunk Service Number | Enter the trunk service number that identifies a line in the Trunk Attributes form which determines the desired incoming characteristics for the XNET trunk (rather than using the trunk service of the actual physical trunks involved in the call). Valid numbers are 1 to the maximum trunk service number at this system. The Trunk Service Number must be programmed in the Trunk Attributes form before it can be used in this form. | Blank
Interconnect Number | Enter a number between 1 and 64, which is used in the Interconnect Restriction Table to define the other devices that the XNET trunk may connect to (rather than using the interconnect restrictions of the actual physical trunks involved in the call). The Interconnect Number must be programmed in the Interconnect Restriction Table before it can be used in this form. | Blank
Remote Profile Number | Enter the number that corresponds to the Local Profile Number field in the XNET Trunk Profiles form at the Remote system; it has the desired trunk service and interconnect characteristics (compatible with the Local Profile Number profile at this system.) Valid numbers are 1 to 81. | Blank
Comments | Enter information (up to 16 characters) to identify the characteristics associated with the profile. | Blank