# Programming Analog Sets and Trunks on an AX Controller

## Before You Begin

You must purchase an analog line license for each ONS port on a 24 Port ONSP Card, 16 Port ONS Card, and 4 + 12 Port Combo Card. Check the Analog Line Licenses fields in the System Capacity form ( ) to determine the number of available licenses. Subtract the number of used licenses from the number of purchased licenses.

## Programming

To program analog sets and analog trunks in an AX controller:

1. Analog Services Units form

- Configure the AX Controller card chassis:

- Click Change.

- Select "AX Card Chassis" from the Programmed Type field.

- Enter a number between 2 and 16 in the Unit field.

- Click Save.

2. Card Assignment form

- Select the appropriate programmed card type. The only valid card types are 24 Port ONSP Card, 16 Port ONS Card, 16 Port ONS Card and 4 + 12 Port Combo Card.

3. Program the analog telephones, analog trunks, Music on Hold, and Paging:

4. Program Analog Telephones

5. Program Analog Trunks

6. Program Music On Hold

Related Topics

- About the AX Controller