# HST STATUS_HANDOFF

## Qualifiers:

None

## Purpose:

Use this command to display the status of the HST Courtesy_Handoff command.

## Details:

Use the HST STATUS_HANDOFF command on the controller on which you initiated the HST Courtesy_Handof command.

## Example:

### Entry: HST STATUS_HANDOFF

### System Response:

Index | Dest PBXNum | HealthCheck? | #OKChecks | #Devices | Devices Handoff To
0 | 11 | True | 0 | 102 | SICP

Where:

Dest PBXNum means Cluster element ID

HealthCheck? means "Is health checking active for the destination ICP?" - (True/False)

#OKChecks means Number of good health checks received

#Devices means Number of devices to be transferred to the other ICP

Devices Handoff To means SICP, PICP (in the case of transferring back to the Primary ICP) and SICP + PICP (both)

Related Topics

- HST Courtesy_Handoff

- HST CANCEL_HANDOFF