# DSP II Alarm

## System/Sub-System

MiVoice Business: Hardware

## Description

There is an FPGA firmware version mismatch on a DSP II card.

## Alarm Status

The major threshold is 100%.

#### Possible Cause | #### Corrective Action
--- | ---
Hard disk or DSP II card replacement. | Enter the UPGRADEBOOTROM ALL maintenance command to upgrade the firmware. You MUST reset the system to have the upgraded firmware take effect.