# Remote Busy Lamps

## Purpose

The Remote Busy Lamps form allows you to program remote appearances of a local device. The form lists the device's local appearances as programmed in the Multiline Set Keys form and allows you to enter remote directory numbers of devices that will host a busy lamp appearance of the local device.

Use this form when performing the following tasks:

- Direct Station Selection/Busy Lamp Field (DSS/BLF)

## Field Descriptions

Parameter | Description | Default Value
Monitored Device | The directory number of the local single-line set or Broadcast Group A directory number programmed to appear on multiple devices constitutes a broadcast group. There are two types of broadcast groups: Non-Prime Line and Prime Line. A Non-Prime Line group is a directory number programmed on one or more devices that is not the prime line on any device. A Prime Line group is a directory number programmed on button 0 of a phone. Server-based variants of MiVoice Business that use x86 processors, MiVoice Business for Industry Standard Servers MCD-ISS), Multi-instance MiVoice Business, and Virtual MiVoice Business, up to 250 appearances of the directory number can appear on one or more devices. For all other 3300 ICP/MiVoice Business call control platforms, up to 32 appearances of the directory number may appear on one or more devices. that is being monitored on a remote device. Entering a remote directory number in this field will display all local busy lamps programmed against the remote device or group. | Blank
Local Host Set Directory Number - n | The directory number(s) of devices that have appearances of the monitored device. |
Name | System-generated, protected field. Provides the name assigned to the directory number in the Telephone Directory form. |
Remote Lamp | System-generated, protected field. An index number used internally to identify instances of the monitored DN. |
Remote Host Set Directory Number | The remote directory number of the devices that will host busy lamps for monitoring the local device or group. Local and remote busy lamp appearances of the monitored device must total no more than 64. | Blank