# Programming Programmable Key Modules

## Before You Begin

This procedure is applicable to PKM 12, PKM 48, Dual PKM, and PKM 695 modules.

NOTES

- Before connecting the PKM, ensure that the appropriate PKM Interface Module is installed in the phone. After you connect the PKM, you must reboot the IP Phone before you program the PKM keys.

- To support a dual PKM, the phone must have an H2 hardware revision with main load of 9.4 and a boot load of 9.3 or later.

## Programming

To program a PKM Module:

1. Multiline IP Sets form ( )

- IP Phone: select the telephone that the PKM will attach to, click Change and select "PKM 12", "PKM 48", "Dual PKM" or "PKM 695" in the Auxiliary Module field.

2. Multiline Set Keys form

- Program the keys.

NOTE: The three fixed keys on the Mitel M695 Programmable Key Module (PKM) is supported for use by MiVoice Business.