# VM RAD Greetings

## Purpose

The VM Recorded Announcement Device (RAD) Greetings form is used to manage greeting sets. Up to 30 RAD greeting sets (10–39) can be created, with 1 to 5 greetings per set.

Use this form when performing the following tasks:

- RAD Greetings

## Field Descriptions

Parameter | Description | Default Value
RAD Set | System-generated. The identification number of the RAD greeting set. |
Greeting n | Enter a number in the range 1 to 200 that corresponds to the greeting that you want played in this position. Numbers are assigned to greetings at the time of recording or downloading via the System Audio Source Update form. A greeting can belong to more than one set. A set can have multiple instances of the same greeting. | Blank
Times To Play | Enter how many times the greeting set plays before the port closes. | Blank

Greeting 1: Enter a number in the range 1 to 200 that corresponds to the greeting that you want played in this position. A greeting can belong to more than one set. A set can have multiple instances of the same greeting.

Greeting 2: Enter a number in the range 1 to 200 that corresponds to the greeting that you want played in this position. A greeting can belong to more than one set. A set can have multiple instances of the same greeting.

Greeting 3: Enter a number in the range 1 to 200 that corresponds to the greeting that you want played in this position. A greeting can belong to more than one set. A set can have multiple instances of the same greeting.

Greeting 4: Enter a number in the range 1 to 200 that corresponds to the greeting that you want played in this position. A greeting can belong to more than one set. A set can have multiple instances of the same greeting.

Greeting 5: Enter a number in the range 1 to 200 that corresponds to the greeting that you want played in this position. A greeting can belong to more than one set. A set can have multiple instances of the same greeting.