# Single Line IP Sets

## Purpose

The Single Line IP Sets form is for programming the 5001 and 5201 single-line IP phones. The form supports Range programming.

Use this form when performing the following tasks:

- Program Single Line IP Telephones

## Conditions

- When deleting IP sets, you must also delete the corresponding directory entries and voice mailboxes.

## Field Descriptions

Parameter | Description | Default Value
Device Id | System-generated, protected field. Lists the programmed Device ID. |
Device Type | Select the attached device type. | 5001 IP
Number | Enter a unique number up to seven digits in length to be assigned to the line circuit. This is the number dialed to ring the telephone. | Blank
Local-only DN | Allows you to specify the directory number as a local-only directory number in a cluster. | Not Selected
Interconnect Number | Enter a number, between 1 and 64, that references an entry in the Interconnect Restriction form. | Blank
Non-busy Extension | Select "Yes" to indicate that the associated extension is a non-busy extension; leave the entry at No to indicate that the set is a regular extension. A non-busy extension requires a COS that has the conference option enabled. | No
MAC Address | Enter the Media Access Control identifier for the IP telephone. | Blank
Tenant Number | Enter the number of the set's tenant. | 1 (landlord)
User PIN | Enter a password for the hot desk user, SIP Phone user, or the Phone Lock feature. This field is available if the Hot Desk User or Generic SIP User field is set to "Yes". The PIN can only include digits from 0 to 9 and can be from 0 to 10 digits in length. | Blank
Confirm User PIN | Re-enter the password to confirm. | Blank
Service Level | System-generated, protected field. Identifies the Service Level assigned in the User and Services Configuration form. NOTE: All devices added on this form have Full Service This Service Level indicates that the directory number (DN) is assigned to a standard user and device with full telephony functionality.. Use the User and Services Configuration form to program other Service Levels. |