# Dialing - Conflicting Numbers

## Description

The system can differentiate between conflicting numbers, such as 1-0-0-0-0 and 1-0-0-0. In this example, if the 5th digit is not dialed within a time-out period, the system assumes that the dialed sequence is complete and makes the call.

## Conditions and Feature Interactions

None

## Programming

- Class of Service Options form

- Program the dialing conflict timer value. Make it less than the interdigit timer value.

## Device Support

Not applicable

## Operation

None