# Embedded Voice Mail - Default Settings

Parameter | Default Setting
Default Digit length for mailbox | 4 digits
Maximum number of messages per mailbox | 50
Administrator mailbox | Mailbox: 9999. Password: none (to log in, you must first set up the Admin, Manager and Technician passcodes in the VM Options form)
Bilingual Option | Enabled (checked). Default primary and secondary languages determined by the country variant selected in Software Installer during installation or in the License and Options form.
Auto Attendant Transfer method | Unsupervised
System Routine Maintenance | Daily at 3 A.M. Note: Voice mail is out of service for approximately 3 minutes.
Number of voice mail ports | 30 for all x86 (server) platforms 20 for all PowerPC (3300 ICP) platforms

NOTE: If the mailbox digit length and directory number digit length are different, you cannot edit mailboxes using the Group Administration Tool (you can still use the System Administration Tool and the Administrator's Mailbox). To change the mailbox digit length, perform a New Installation from the Administrator's Mailbox (this will erase the voice mail database).

Related Topics

- About Embedded Voice Mail

- Additional Documentation

- Capacities

- Program Embedded Voice Mail