# RESOURCE

## Qualifiers:

<unit> <shelf> <slot> <circuit or hybrid>

<unit> <shelf> <slot> <circuit or hybrid> <channel>

XNET <trunk>

## Purpose:

Displays information about the resources used by the call process which owns a specified circuit.

## Details:

A Resource display may only be requested for a single circuit and that circuit must be participating in an active Call Process.

The command is valid for DTMF circuits only.

The <channel> qualifier allows the resources used by a specific channel on a CEPT or DS1 Formatter card to be displayed.

The <hybrid> qualifier is used to specify hybrid 1 or 2 on a CEPT or DS1 Formatter card. If no qualifier is used, both are displayed.

The XNET qualifier accommodates XNET trunks (which do not have a PLID). A device type of "XNET Trunk" is displayed when the resource is requested for a trunk, set, or console being used in an XNET call.

Resources Command Printout Headings (See Examples)
Field | Description
Circuit: | Type of circuit (line or trunk) specified.
Call Process: | Call Process that owns circuit specified in the command.
Device Type: | Type of device used by Call Process, such as: Attendant Console IP Telephone Trunk Type. NOTE: The 5320/5320e, 5330/5330e, 5340/5340e and 5360 IP Phones show up as a 4025 IP.
Digit Receiver: | DTMF Receiver in use.
Call State | State of call in progress (see following table).
Party Type | Originator, Terminator, or Nil Party Type.
Receive Link | Link number of allocated PCM receive channel.
Receive Channel | Allocated PCM receive channel number.
Transmit Link | Link number of allocated PCM transmit channel.
Transmit Channel | Allocated PCM transmit channel number.

NOTES

1. "Device Type" for the "Party Type" Terminator is irrelevant to Call Processing Software and is not displayed.

2. "Digit Receiver" field is included only when either party is using, or has yet to release a DTMF receiver.

Call States
State | Definition
Dialing Party | Party is dialing a number.
Hard Hold | Party placed on hole via 'flash switchhook' followed by a feature code by the other party.
Idle | Initial State.
In Use | Modem Tone.
In Lock Out | All resources have been releases and party must hang up and start over.
Listen to Answer | Modem tone.
Listen to Busy | Party has called another party already involved in a call and is listening to the applicable tone.
Listen to Camp on | Party has camped-on to a busy party and is listening to a confirmation tone indicating the camp on was successful.
Listen to DND | Party has called another party that has a Do Not Disturb feature and is listening to the applicable tone.
Listen to Reorder | The party's attempt to make a call or invoke a feature has failed, and they are receiving the indication to start over.
Overriding Party | Party is performing a busy override.
Outpulsing Digits | Party is calling another party outside of this PBX and is outpulsing digits to a trunk.
Releasing Party | Party is being cleared down.
Ringing | Device is ringing.
Seizure Party | Ringing is being initiated on the party.
Soft Hold | Party placed on hold via 'flash switchhook' or feature activation by other party.
Talking | Voice connection exists between this party and another.
Waiting for Answer | Party is listening to ringing.
Waiting for Pickup | Party has dialed and is waiting for ringing (or busy, etc.) to commence.

## Examples:

### Entry: RESOURCE XNET 5

System Response:

Circuit: XNet Trunk ID 5
Call Process: 2 501 Call State: Talking Receive Link: 128 Channel: 0 | Device Type: Dig Dial in Trnk Party Type: Terminator Transmit Link: 128 Channel: 0
>>>>>>Other Party for Call Process 2 501
Circuit: Line at location 1 3 1 7 1
Call Process: 3 502 Call State: Talking Receive Link: 53 Channel: 6 | Device Type:5020 IP Party Type: Originator Transmit Link: 53 Channel: 6
>>>>>>Signaling Device for Call Process 2 501
Circuit: MCSTHA ICP Comms at location 1 1 11 3
Owner Process: 2 599 Link Handle: A | State: Established Remote PBX ID: 167
>>>>>>Traffic Channel for Call Process 2 501
**** Undefined Call Record ****

### Entry: RESOURCE 1 3 1 7 1

System Response:

Circuit: Line at location 1 3 1 7 1
Call Process: 5 504 Call State: Talking Receive Link: 51 Channel: 4 | Device Type:5020 IP Party Type: Originator Transmit Link: 51 Channel: 4
>>>>>>Other Party for Call Process 5 504
Circuit: MC330AA Line at location 1 3 1 9 1
Call Process: 4 503 Call State: Talking Receive Link: 52 Channel: 5 | Device Type:5020 IP Party Type: Terminator Transmit Link: 52 Channel: 5