# T38 Load Fail Alarm

## System/Sub-System

MiVoice Business: Software

## Description

Indicates an issue with the T.38 software/hardware/configuration (including licensing) on system startup.

## Alarm Status

The minor threshold is 100. The major threshold is 100.

#### Possible Cause | #### Corrective Action
--- | ---
T.38 licensed without DSP II being installed. DSP II card failure. DSP II card is installed in the wrong slot. | Use slotallinfo maintenance command to determine if DSP II card is installed. Replace DSP II card. Ensure DSP II card is installed in slots 4,5, or 6 of MXE controller.