# Trunk Labels

## Description

Trunk Labels may be assigned to individual trunks or groups of trunks. When a trunk call appears at an attendant console, the trunk label and trunk number are displayed.

Trunk labels operate differently depending on the device and its state.

Trunk with Trunk Label
Device Type | Ringing | Answered
IP Console Applications(MiVoice Business Console) 5540 IP Console | Associated LDN | Trunk label and number
5010 IP Phone 5020 IP Phone 5140 IP Phone 5220 IP Phone 5220 IP Phone (Dual Mode) 5224 IP Phone 5324 IP Phone 5240 IP Phone 5320/5320e IP Phone 5330/5330e IP Phone 5340/5340e IP Phone 5360 IP Phone 69xx IP Phones Navigator | Trunk label Calling | Trunk label

## Conditions and Feature Interactions

- Several trunk service numbers may have the same label.

- Trunk Labels are typically used in multi-tenant applications.

## Programming

- Trunk Attributes form

- Program a Trunk Label.

## Device Support

- Supported on all devices.

## Operation

None