# Programming an IP Paging Unit

## Before You Begin

For the Mitel IP paging unit to boot up, DHCP options 128-133 must be programmed in the DHCP server. After the sets have booted, options 128-133 may be removed to avoid future conflicts with standard use or other vendors use of these options.

## Programming

To program a Mitel IP Paging Unit (this procedure will produce a ring burst at the beginning of each page):

1. Multiline IP Sets form

- Program the IP Paging Unit as "5010 IP".

- Enter the MAC address.

2. (Optional) Feature Access Codes form

- Assign a code to Direct Page Paging.

3. (Optional) Multiline Set Keys form

- Program a Paging key.

4. Interconnect Restriction form

- Ensure that the station is not restricted from Paging.

To program Group Page with the IP Paging Unit (This programming procedure will ensure that a ring burst does not occur prior to the speech broadcast):

1. Multiline IP Sets form

- Program the IP Paging Unit as "5010 IP".

- Program the MAC address.

2. Page Groups form

- Complete all required fields.

NOTE: Symbol Wireless Phones should not be programmed into paging groups.

3. Class of Service Options form

- Set the Group Page Accept field to "Yes" for the IP Paging Unit.

- Ensure that each telephone in the paging group has the Group Page Allow field set to "Yes".

4. (Optional) Feature Access Codes form

- Assign a Direct Page feature access code.

5. (Optional) Multiline Set Keys form

- Program a Paging key.

6. Interconnect Restriction form

- Ensure that the station is not restricted from Paging.