# Direct Outward Dialing (DOD)

## Description

Direct Outward Dialing (DOD) lets you make external calls without the assistance of the attendant.

## Conditions and Feature Interactions

None

## Programming

- ARS Leading Digits form

- Program the Leading Digits (typically "9").

## Device Support

All devices

## Operation

To use Direct Outward Dialing:

1. Lift the handset.

2. Dial the Leading Digits.

3. Dial the destination digits.