# Program ARS Routes Between the Cluster Elements

Program the ARS at each element. Using the CEID digits as ARS leading digits, program ARS to route calls to each of the other remote elements. Note that the ARS routing digits (CEID digits + extension number) on each element in the cluster must be the same length. For an example, see Figure 1 below.

Proceed to Program IP Network and XNET Trunks.

Figure 1: ARS Route Programming Example