# HST CANCEL_HANDOFF

## Qualifiers:

None

## Purpose:

Use this command to cancel the HST COURTESY_HANDOFF command.

After you enter this command on the primary controller

1. Any IP resilient sets that have not already been handed off to the secondary remain on the primary controller.

2. Any IP resilient sets that have already been handed off to the secondary controller are sent back to the primary controller. This is not instantaneous, but all the sets will be sent back over time.

## Details:

- You must enter this command on the primary controller.

- You will not see an error message if you enter this command on the secondary controller, but there will be no effect.

- As the Cancel operation is being completed, the Primary ICP will respond to health checks sent by the Secondary ICP.

## Example:

### Entry: HST CANCEL_HANDOFF

### System Response:

Sending CANCEL_HANDOFF Msg .........

Related Topics

- HST Courtesy_Handoff

- HST Status_Handoff