# SHOW FAULTS

## Qualifiers:

<alarm category>

ALARMS

## Purpose:

Provides a list of all the faults that are responsible for the alarm status.

## Details:

The ALARMS qualifier provides a list of faults for all those alarm categories that have alarms raised.

NOTE: IP125Ax IP Line in the Card Description column indicates the part number of IP phone circuit.

## Examples:

### Entry: SHOW FAULTS ALARMS

System Response:

Digital Links
Cab, Shelf, Slot | Card Description | Total Faults
6 1 1 | MC270AX Universal T1 | 1

System Response:

No faults for specified alarm category

### Entry: SHOW FAULTS TRUNKS

System Response:

Cab | Shelf | Slot | Card Description | Total Faults
7 | 1 | 4 | MC263AX DS1 formatter | 48