# Current Bandwidth Statistics

## Purpose

This form allows you to display current statistics related to zone access points (ZAPs) managed by the local MiVoice Business system.

Use this form to perform the following tasks:

- Program Bandwidth Management

- Network Zone Topology

- Display Bandwidth Historical 15 Minute

- Using Bandwidth Statistics

- Setting Bandwidth Alarm Thresholds

For more information about Bandwidth Management:

- Bandwidth Management - Introduction

## Conditions

None

## Field Descriptions

Parameter | Description
Zone ID | The zones (1 to 999) listed in the Network Zone Topology form.
Parent Zone ID | The parent zone in the zone tree
Zone Access Point ID | The ID (1-6) of the ZAP.
Zone Access Point Label | The label of the ZAP.
Bandwidth In Use (kbit/s) | The bandwidth in use at the ZAP.
Bandwidth Limit (kbit/s) | The bandwidth limit for the Zone Access Point. The minimum bandwidth is 1 kbit/s (1024 bits per second) and the maximum bandwidth is 1 Tbit/s (1,099,511,627,776 bits per second).
CAC Admissions | The number of calls admitted through ZAP since the ZAP was created or system startup
CAC Rejections | The number of calls rejected because bandwidth was fully utilized through ZAP since the ZAP was created or system startup.