# Network Specific Facilities Dependencies

Protocol | Variant | Applicable Options
DMS-100 DMS-250 |  | Unassigned Default Private FX Tie Trunk Outwats
4ESS |  | Unassigned Default SDN Megacom Accunet
NI-2 | Bellcore | Unassigned Default FX Tie Trunk Unb. OW Band. OW
NI-2 | 5ESS | Unassigned Default FX Tie Trunk Accunet Unb. OW Band. OW (not for fixed) VPN ( SDN) WATS Max Int LDS ETN PVN WATS Bnd (not for fixed)
NI-2 | GTD5 | Unassigned Default FX Tie Trunk Und. OW Band. OW (not for fixed)