# Transfer to a Busy Device (TI/D4)

The Transfer to a Busy Device feature allows a user to transfer an incoming trunk or station across the network to a busy device. The transferred party is automatically camped-on to the busy device when the party who invoked the transfer hangs up. Camp-on is not possible if the called station has Do Not Disturb activated.

This feature is not subject to conditions, programming, or operation instructions.