# SFT Zones Alarm

## System/Sub-System

MiVoice Business: Software

## Description

System Fail Transfer (SFT) zones have switched into SFT mode.

Maintenance commands are valid for this alarm.

## Alarm Status

The major threshold is > 0. The critical threshold is 100.

#### Possible Cause | #### Corrective Action
--- | ---
System Fail Transfer zones have switched into SFT mode. | Determine cause for switch to SFT mode.