# Card Assignment

## Purpose

Use the Card Assignment form to program each card supported by the AX Controller Peripheral Services.

The AX Controller supports up to 12 analog cards with up to 288 ports; the ASU II supports up to 2 analog cards with up to 48 ports. Valid card types for the AX Controller and ASU II are the 24 Port ONSP Card, 16 Port ONS Card, and 4 + 12 Port Combo Card.

Use this form to perform the following tasks:

- Program Analog Sets and Trunks on an AX

## Conditions

- This form does not apply to the CX II or CXi II controller.

## Field Descriptions

Parameter | Description | Default Value
Cabinet | System-generated, protected field indicating the location of the card in the system. |
Shelf | System-generated, protected field indicating the location of the card in the system. |
Slot | System-generated, protected field indicating the location of the card in the system. |
Programmed Card Type | Select the appropriate programmed card type (this may vary among cards within the same cabinet). | No Card
Installed Card Type | System-generated, protected field. Lists the installed card type at this location. |