# Ringing Line Select

## Description

Ringing Line Select lets you answer any ringing line by going off-hook.

If several lines are ringing, you will answer ringing lines in the following order:

1. Ringing or flashing prime line.

2. Ringing or flashing single line (descending priority from the bottom key to the top key).

3. Ringing (not flashing) non-prime Broadcast Group
   A directory number programmed to appear on multiple devices constitutes a broadcast group. There are two types of broadcast groups: Non-Prime Line and Prime Line. A Non-Prime Line group is a directory number programmed on one or more devices that is not the prime line on any device. A Prime Line group is a directory number programmed on button 0 of a phone. Server-based variants of MiVoice Business that use x86 processors, MiVoice Business for Industry Standard Servers MCD-ISS), Multi-instance MiVoice Business, and Virtual MiVoice Business, up to 250 appearances of the directory number can appear on one or more devices. For all other 3300 ICP/MiVoice Business call control platforms, up to 32 appearances of the directory number may appear on one or more devices. line (descending priority from bottom key to top key).

## Conditions and Feature Interactions

The Ringing Line Select COS does not apply to the prime line or the non-prime single line. For more information see Line Types and Appearances.

## Programming

- Class of Service Options form

- Set Ringing Line Select to YES.

## Device Support

- Supported on all devices.

## Operation

#### All telephones

To answer a call when you hear ringing:

- Lift the handset.