# Programming a MiVoice Business System as a Standalone Voice Mail Server

## Overview

The MiVoice Business voice mail application can be used as a standalone voice mail server behind any PBX that has DPNSS or QSIG trunks.

## Programming

To program a MiVoice Business system as a standalone voice mail server:

1. License and Option Selection form

2. Program the number of digital links, voice mail licenses, and country variant.

2. Reboot To reboot the system, press the Reset button on the Controller.
   the system.

5. Program digital trunks QSIG or MSDN/DPNSS.

6. Program voice mail.

Related Topics

- About Embedded Voice Mail

- Detailed Voice Mail Description

- Additional Documentation

- Capacities

- Default Settings

- Program Embedded Voice Mail