# Gateway Trunk Profiles (EX Controller)

## Purpose:

The Gateway Trunk Profiles form is used to create Gateway Trunk Profiles for the EX Controller. This form helps create logical grouping of the gateway trunks. You must create a profile before EX Controller trunks can be used. When the EX Controller is added to the MiVoice Business system using the Enterprise Gateways form, a trunk profile is created for each type of trunk on the EX Controller.

NOTE: This form is applicable only to the EX Controller.

Use this form when performing the following tasks:

- Add Gateway Trunk Profiles

- Change Gateway Trunk Profiles

- Delete Gateway Trunk Profiles

## Conditions

- If there are ONS cards in the system, a maximum of four SIP Peer gateway trunk profiles can be created. Otherwise, a maximum of five trunk profiles can be created using the Gateway Trunk Profiles form.

- The Gateway Trunk Profile records are related to the SIP Peer network element records of the Network Elements form. But the changes made to SIP Peer Port in the Network Elements form will not update the associated Gateway Trunk Profile.

## Field Descriptions

Parameter | Description | Default Value
Gateway Trunk Profiles
Gateway | Indicates the IP address of the gateway that is programmed for the EX Controller. | Not applicable
Name | Enter a name (maximum of 9 characters) for the gateway profile. | Blank
Zone | Enter the zone number (between 1 and 999) for the gateway trunk profile. | 1
SIP Peer Port | Read-only. Indicates the port number for the SIP peer. The SIP Peer Port will be automatically assigned from a port number in the range 5062-5066 |
Trunk Attributes
Trunk Service Number | Enter a trunk service number (between 1 and 500). | Blank
Class of Service | Enter a Class of Service (COS) number (between 1 and 110). | 1
Class of Restriction | Enter a Class or Restriction (COR) number (between 1 and 110). | 1
Non-dial In Trunks Answer Point - Day | Enter a trunk answer point number (maximum of seven digits). | Blank
Non-dial In Trunks Answer Point - Night 1 | Enter a trunk answer point number (maximum of seven digits). | Blank
Non-dial In Trunks Answer Point - Night 2 | Enter a trunk answer point number (maximum of seven digits). | Blank
Dial In Trunks Incoming Digit Modification - Absorb | Enter a digit modification number (maximum of 26 digits). | Blank
Dial In Trunks Incoming Digit Modification - Insert | Enter a digit modification number (maximum of seven digits). | Blank
NOTE: The Non-dial In Trunks Answer Point fields and Dial In Trunks Incoming Digit Modification fields are mutually exclusive and cannot be configured at the same time.
Incoming DID Range | Enter a DID range (maximum of 60 characters). | Blank
SIP Peer Profile
Default CPN | Indicates the called party number (maximum of 26 characters). | Blank