# SLOTALLINFO

## Qualifiers:

None

## Purpose:

Use this command to show the type of card installed in each slot in the system.

## Example:

### Entry: SLOTALLINFO

System Response:

Info returned by SystemDiscovery:: MmcInfo():

MMC slotID : 0

moduleid : 12

driverid : 1

resetTiming : 0

pcbAssembly : 56001801

pcbRev : RA

variant Id : 0

describ :

country code :

procType :

coreSpeed : 0

clockSpeed : 0

pasicID : 4

controllerID : 0

IRQ levels : 2

8b Base Addr: 0x40000000

16b Base Addr: 0x50000000

32b Base Addr: 0x60000000

MAC Address :

> no MMC module detected in slot 1

> no MMC module detected in slot 2

MMC slotID : 3

moduleid : 47

driverid : 6

resetTiming : 100

pcbAssembly :

pcbRev :

variant Id : 0

describ : 4 SHARC 21161 DSP

country code :

procType : ADSP 21161N

coreSpeed : 100

clockSpeed : 25

pasicID : 4

controllerID : 0

IRQ levels : 2

8b Base Addr: 0x46000000

16b Base Addr: 0x56000000

32b Base Addr: 0x66000000

MAC Address :

> no MMC module detected in slot 4