# System Log Messages
(Embedded Voice Mail)

The System Log records unusual activities within in the system. The voice mail portion of the log has five fields:

DATE TIME LEVEL MSG#-PORT MESSAGE

- DATE and TIME indicate when the event occurred.

- LEVEL indicates the message category and therefore the level setting required to include such messages in the output stream.

0 = FATAL (voice mail system shuts down)

1 = ERROR (abnormal event)

2 = WARNING (may be an abnormal event)

3 = INFO (normal monitoring)

4 = TRACE (detailed monitoring, intended for lab use only)

5= DEBUG (very low-level, intended for lab use only)

- MSG# is a unique identifier for each message.

- PORT is the single-digit voice mail port associated with the message (or 0 if not port-specific).

- MESSAGE provides text indicating the event.

Click Details for additional information on error numbers.